0x01>Open device handle fail (01)>Can't get device handle
0x02>Allocate memory fail (02)>Can't allocate some buffers to start initial card thread
0x08>Check FW RunMode fail (08)>Vendor command flow fail when check mode
0x09>Read Parameter Table fail (09.01)>Vendor command flow fail when read parameter table
0x09>Read Parameter Table fail (09.02)>Can't find parameter table string tag
0x09>Read Parameter Table fail (09.03)>Can't find FlashID information
0x0A>Read IDTable fail (0A)>Vendor command flow fail when read ID table
0x0B>Keep Serial number fail (0B)>Can't get serial number from Idtable or MPInfo
0x0C>Read MPInfo fail (0C)>Vendor command flow fail when read MPInfo
0x0D>Check ChangeID flag fail (0D.01)>Vendor command flow fail when read parameter table
0x0D>Check ChangeID flag fail (0D.03)>Wrong Parameter Table
0x0E>Read CID fail (0E)>Vendor Command flow fail at ReadCID
0x0F>Compare Flash Fail (0F)>Flash name is not matched with FlashDB
0x10>Download MPISP fail (10)>Allocate memory fail when download MPISP procedure
0x11>Download MPISP fail (11)/(04.02)>Vendor command flow fail when force to RomCode mode 
0x11>Download MPISP fail (11)/(06.02)>Vendor command flow fail when download code
0x11>Download MPISP fail (11)/(06.03)>Vendor command flow fail when check mode
0x11>Download MPISP fail (11)/(06.04)>Vendor command flow fail when reset cpu
0x13>Read FlashID fail after download MPISP (13)>Vendor command flow fail when Read FlashID
0x14>Can't support this unbalanced configuration (14)>Unbalanced configuration is not matched standard
0x15>Can't support multi-die unbalanced mode (15)>Don't support multi-die unbalanced case
0x16>Can't support this multi-die unbalanced configuration (16)>Now, just support final CE lost final die case
0x17>Compare Flash Fail (17)>FlashID is not matched with FlashDB
0x18>GPIO Check fail (18)/(3C.01)>Check setting about Toggle pin
0x18>GPIO Check fail (18)/(3C.02)>Check setting about Reliable pin
0x18>GPIO Check fail (18)/(3C.03)>Vendor command flow fail
0x18>GPIO Check fail (18)/(3C.04)>Check setting about AleExtend pin
0x19>Channel0-CE0 didn't exist flash (19)>Don't support this flash layout
0x1A>Check MPISP Mode fail (1A)>Vendor command flow fail
0x1B>Not MPISP Mode (1B)>Not MPISP mode
0x1C>Check SanDisk Bics Read Retry fail (1C)/(3B.01)>Vendor command flow fail
0x1D>Some die didn't support RR function (1D)>Some die didn't support Read Retry function
0x1E>Read B16/B17 Grade fail (1E)/(3A.01)>Vendor command flow fail
0x1F>Flash Mixed Different Grade (1F)>Mixed different grade flash
0x20>Dump system block fail (20)/(13.01)>Load Parameter table fail
0x20>Dump system block fail (20)/(13.02)>Vendor command flow fail when read flash page
0x20>Dump system block fail (20)/(13.03)>Dump all Info Block fail
0x20>Dump system block fail (20)/(13.04)>Dump all ISP Block fail
0x20>Dump system block fail (20)/(13.05)>Dump BadInfo Block occur ECC fail
0x21>SRAM Test fail (21)/(07.01)>Vendor command flow fail
0x21>SRAM Test fail (21)/(07.02)>SRAM test fail
0x22>Flash Connectivity Test fail (22)/(08.0A)>Vendor command flow fail when Read FlashID
0x22>Flash Connectivity Test fail (22)/(08.0B)>Vendor command flow fail when Read Connectivity Test
0x22>Flash Connectivity Test fail (22)/(08.12)>FlashID differece with FlashDB
0x23>Generate CH/CE Map fail (23)/(0E.01)>The number of Ch or Ce is zero
0x23>Generate CH/CE Map fail (23)/(0E.0C)>Die Num per Ce are different with DataBase
0x23>Generate CH/CE Map fail (23)/(0E.0D)>Ce location per Ch are different
0x23>Generate CH/CE Map fail (23)/(0E.0E)>CeMap mismatch setting
0x23>Generate CH/CE Map fail (23)/(0E.0F)>ChMap mismatch setting
0x24>Build Parameter Table fail (24)/(12.27)>It's not TLC flash
0x24>Build Parameter Table fail (24)/(12.28)>Check parameter table correctness fail
0x25>Set CardMode fail (25)/(26.01)>Vendor command flow fail
0x25>Set CardMode fail (25)/(26.02)>Transform L06B to B0KB fail
0x26>TranRTC fail (26)>Vendor command flow fail (Dll function)
0x27>TranADJ fail (27)/(0C.01)>No Good Window for Read
0x27>TranADJ fail (27)/(0C.02)>No Good Window for Program
0x27>TranADJ fail (27)/(0C.03)>Program all fail in Tran Read Dll
0x27>TranADJ fail (27)/(0C.04)>Read all fail in Tran Read Dll
0x27>TranADJ fail (27)/(0C.05)>Program all fail in Tran Program Dll
0x27>TranADJ fail (27)/(0C.06)>Read all fail in Tran Program Dll
0x27>TranADJ fail (27)/(0C.07)>Tran interface failed
0x2A>Get LastTimeBad fail (2A)>Buffer offset is overflow, maybe InfoBlock information error
0x2B>Get RunTimeBad fail (2B.01)>TotalRunTimeBad Count is Zero
0x2B>Get RunTimeBad fail (2B.02)>TotalRunTimeBad Count is too large
0x2B>Get RunTimeBad fail (2B.03)>Fblock index is overflow range
0x2D>Get LastTimeBad fail (2D)/(39.01)>InfoTotalBlkStatusAddr size wrong
0x2D>Get LastTimeBad fail (2D)/(39.02)>InfoTotalBlkFinalAddr size wrong
0x2E>Get RunTimeBad fail (2E)/(38.01)>Failed in PtestGetDumpRuntimeBadStatus
0x2E>Get RunTimeBad fail (2E)/(38.02)>TotalRunTimeBadPtrCnt Overflow
0x2E>Get RunTimeBad fail (2E)/(38.03)>BadInfoFBlkOffset Overflow
0x2F>Shallow Erase check fail (2F)/(3D.01)>Vendor command flow fail
0x2F>Mixed Shallow Erase (2F)/(3D.02)>Sample mixed fail
0x2F>Shallow Erase check fail (2F)/(3D.03)>Parameter page read fail and Sample not mixed
0x2F>Mixed Shallow Erase (2F)/(3D.03)>Parameter page read fail and Sample mixed
0x30>Scan OriginalBad fail (30)/(30.01)>Nand flash timeout when read cmd
0x30>Scan OriginalBad fail (30)/(30.02)>Block address is overflow
0x30>Scan OriginalBad fail (30)/(30.03)>Block address is error
0x30>Scan OriginalBad fail (30)/(30.04)>Maybe the SRAM problem, please check TSB SRAM!!
0x30>Scan OriginalBad fail (30)/(30.05)>ScanBad Mode setting wrong
0x32>Sort EraseBad fail (32)/(32.01)>Nand flash timeout when erase cmd
0x32>Sort EraseBad fail (32)/(32.02)>Block address is overflow
0x32>Sort EraseBad fail (32)/(32.03)>Block address is error
0x32>Sort EraseBad fail (32)/(32.04)>Maybe the SRAM problem, please check TSB SRAM!!
0x32>Sort EraseBad fail (32)/(32.05)>Vendor command flow fail when write backup OrgBad info
0x32>Sort EraseBad fail (32)/(32.06)>Write Last SLC Map to SRAM Error
0x34>Program dummy fail (34)/(31.01)>Nand flash timeout when program dummy cmd
0x34>Program dummy fail (34)/(31.02)>Block address is overflow
0x34>Program dummy fail (34)/(31.03)>Block address is error
0x34>Program dummy fail (34)/(31.04)>Maybe the SRAM problem, please check TSB SRAM!!
0x34>Program dummy fail (34)/(31.05)>Vendor command flow fail whe write backup OrgBad info
0x34>Program dummy fail (34)/(31.06)>Write Last SLC Map to SRAM Error
0x40>Set System & Boundary Block fail (40)/(23.01)>System Block Over Rang
0x40>Set System & Boundary Block fail (40)/(23.02)>First Block is different
0x40>Set System & Boundary Block fail (40)/(23.03)>Can't find enough good block to assign system block
0x41>Generate DiffAddr Table fail (41)/(0F.01)>Build SLC DiffAddr Table Fail
0x41>Generate DiffAddr Table fail (41)/(0F.02)>Build TLC DiffAddr Table Fail
0x41>Generate DiffAddr Table fail (41)/(0F.03)>Pick Not Match Fail
0x41>Generate DiffAddr Table fail (41)/(0F.04)>LaterBadCnt Calculate Fail
0x41>Generate DiffAddr Table fail (41)/(0F.05)>Last SLC Block in the TLC range
0x41>Generate DiffAddr Table fail (41)/(0F.06)>First TLC Block in the SLC range
0x41>Generate DiffAddr Table fail (41)/(0F.07)>Extend 8K Diff Table Over Boundary
0x41>Generate DiffAddr Table fail (41)/(0F.09)>Find overlap diff address
0x41>Generate DiffAddr Table fail (41)/(0F.0A)>Physical block address exceed total super block address
0x42>Set Disk Capacity fail (42)/(0D.01)>Manual Capacity Exceed Fail
0x42>Set Disk Capacity fail (42)/(0D.15)>SLC Block is not enough
0x42>Set Disk Capacity fail (42)/(0D.16)>Too much bad block !!
0x43>Calculate Info Block length fail (43)/(10.19)>Get Total Plane of BootISP Fail
0x43>Calculate Info Block length fail (43)/(10.20)>Get Total Plane of Seed Table Fail
0x43>Calculate Info Block length fail (43)/(10.21)>Get Total Plane of Parameter Table Fail
0x43>Calculate Info Block length fail (43)/(10.22)>Get Total Plane of BadBlockStatus Table Fail
0x43>Calculate Info Block length fail (43)/(10.23)>Get Total Plane of BadBlockBitMap Table Fail
0x43>Calculate Info Block length fail (43)/(10.24)>Get Total Plane of DiffType2Bit Table Fail
0x43>Calculate Info Block length fail (43)/(10.25)>Get Total Plane of TotalDiffAddr Table Fail
0x4A>Generate InfoBlk fail (4A)>Dll report info block length is zero
0x4B>Generate InfoBlk fail (4B)>Allocate memory fail when generate Info block procedure
0x4C>Generate InfoBlk fail (4C)/(10.19)>Get Total Plane of BootISP Fail
0x4C>Generate InfoBlk fail (4C)/(10.20)>Get Total Plane of Seed Table Fail
0x4C>Generate InfoBlk fail (4C)/(10.21)>Get Total Plane of Parameter Table Fail
0x4C>Generate InfoBlk fail (4C)/(10.22)>Get Total Plane of BadBlockStatus Table Fail
0x4C>Generate InfoBlk fail (4C)/(10.23)>Get Total Plane of BadBlockBitMap Table Fail
0x4C>Generate InfoBlk fail (4C)/(10.24)>Get Total Plane of DiffType2Bit Table Fail
0x4C>Generate InfoBlk fail (4C)/(10.25)>Get Total Plane of TotalDiffAddr Table Fail
0x4D>Generate InfoBlk fail (4D)/(11.26)>Parameter Table didn't exist 
0x4E>Generate InfoBlk fail (4E)/(24.01)>Vendor command flow fail when Erase Info block
0x4E>Generate InfoBlk fail (4E)/(24.02)>Vendor command flow fail when Program Info block
0x4E>Generate InfoBlk fail (4E)/(24.03)>Vendor command flow fail when Erase Index block
0x4E>Generate InfoBlk fail (4E)/(24.04)>Vendor command flow fail when Program Index block
0x4F>Verify InfoBlk fail (4F)/(24.05)>Calculated checksum is not the same with the one read from nand flash
0x4F>Verify InfoBlk fail (4F)/(24.06)>UNC occurs when reading Info block
0x4F>Verify InfoBlk fail (4F)/(24.07)>Vendor command flow fail when read Info block
0x50>Erase System block fail (50)>Can't translate physical system block index
0x51>Erase System block fail (51)>Vendor command flow fail when Erase system block
0x54>Bin Level not found fail (54)>Bin Level not found fail
0x55>Table not found fail (55)>Table not found fail
0x60>Download ISP fail (60)>Allocate memory fail when download ISP procedure
0x61>Download ISP fail (61)/(25.01)>Vendor command flow fail when Erase ISP block
0x61>Download ISP fail (61)/(25.02)>Vendor command flow fail when Program ISP block
0x61>Download ISP fail (61)/(25.03)>Calculate checksum procedure occur error
0x62>Verify ISP fail (62)/(22.01)>Calculated checksum is not the same with the one read from nand flash
0x62>Verify ISP fail (62)/(22.02)>UNC occurs when reading ISP block
0x62>Verify ISP fail (62)/(22.03)>Vendor command flow fail when check ISP checksum
0x63>Verify ISP fail (63.01)>Vendor command flow fail when write parameter table to SRAM
0x63>Verify ISP fail (63)/(13.01)>Load Parameter table fail
0x63>Verify ISP fail (63)/(13.02)>Vendor command flow fail when read flash page
0x63>Verify ISP fail (63)/(13.03)>Dump all Info Block fail
0x63>Verify ISP fail (63)/(13.04)>Dump all ISP Block fail
0x63>Verify ISP fail (63)/(13.05)>Dump BadInfo Block occur ECC fail
0x63>Verify ISP fail (63.02)>ISP Content is mismatch
0x6A>Download MPInfo fail (6A)/(21.01)>Vendor command flow fail when Erase MPinfo block
0x6A>Download MPInfo fail (6A)/(21.02)>Vendor command flow fail when Program MPinfo block
0x70>Reset Drive fail (70)/(04.04)>Vendor command flow fail when Reset CPU
0x7A>Check ISP Mode fail (7A)>Vendor command flow fail
0x7B>Not ISP Mode (7B)>Not ISP Mode after CPU Reset
0x80>Read Drive Info fail (80)/(0B.01)>Vendor command flow fail when Read Drive Information
0x81>Get Firmware Version fail (81)>Vendor command flow fail when Read ID Table
0xA0>Read RDT Result fail (A0)>Allocate memory fail when get RDT Result procedure
0xA1>Read RDT Result fail (A1)/(35.01)>Seed Table error
0xA1>Read RDT Result fail (A1)/(35.02)>Can't find RDT block
0xA1>Read RDT Result fail (A1)/(35.03)>Vendor command flow fail when Read RDT Result fail
0xA1>Read RDT Result fail (A1)/(35.04)>Read RAM fail, Step1
0xA1>Read RDT Result fail (A1)/(35.05)>Read RAM fail, Step2
0xA1>Read RDT Result fail (A1)/(35.06)>Read RAM fail, Step3
0xA1>Read RDT Result fail (A1)/(35.07)>Read RAM fail, Step4
0xA1>Read RDT Result fail (A1)/(35.08)>RDT Result is Not Trusted
0xA1>Read RDT Result fail (A1)/(35.09)>RDT Timeout
0xA2>RDT Result is not exist (A2)>Can't find "RDT@" string from RDT Result buffer
0xA3>RDT is unfinished (A3)>RDT_PASS flag is Zero
0xA4>RDT Result is FAIL (A4)>RDT_ErrorCode is not Zero
0xA6>Pre-Check Capacity fail (A6)/(0F.01)>Build SLC DiffAddr Table Fail
0xA6>Pre-Check Capacity fail (A6)/(0F.02)>Build TLC DiffAddr Table Fail
0xA6>Pre-Check Capacity fail (A6)/(0F.03)>Pick Not Match Fail
0xA6>Pre-Check Capacity fail (A6)/(0F.04)>LaterBadCnt Calculate Fail
0xA6>Pre-Check Capacity fail (A6)/(0F.05)>Last SLC Block in the TLC range
0xA6>Pre-Check Capacity fail (A6)/(0F.06)>First TLC Block in the SLC range
0xA6>Pre-Check Capacity fail (A6)/(0F.07)>Extend 8K Diff Table Over Boundary
0xA6>Pre-Check Capacity fail (A6)/(0D.01)>Manual Capacity Exceed Fail
0xA6>Pre-Check Capacity fail (A6)/(0D.15)>SLC Block is not enough
0xA6>Pre-Check Capacity fail (A6)/(0D.16)>Too much bad block !!
0xB0>Copy Test fail (B0)>Not ISP Mode before DoCopyCompare procedure
0xB1>Copy Test fail (B1)>Allocate memory fail at CopyCompare procedure
0xB2>Copy Test fail (B2)>Can't allocate memory to dump customize pattern at CopyCompare procedure
0xB3>Copy Test fail (B3)>Read customize file fail at CopyCompare procedure
0xB4>Copy Test fail (B4)>Can't allocate memory to generate random pattern at CopyCompare procedure
0xB5>Copy Test (write) fail (B5)>Write command fail at CopyCompare procedure
0xB6>Copy Test (read) fail (B6)>Read command fail at CopyCompare procedure
0xB7>Copy Test (compare) fail (B7)>Compare data fail at CopyCompare procedure
0xB8>Copy Test (clean) fail (B8)>Clean data fail at CopyCompare procedure
0xC0>[QC]: It's not ISP Mode(C0)>Not ISP Mode before QC procedure
0xC1>[QC]: Read IDTable/MPInfo fail(C1)>Vendor Command flow fail at ReadIDandMPInfo
0xC2>[QC]: MPInfo mismatch, See Log file(C2)>MPInfo(SN+ModelName+WWN8) mismatch user setting
0xC3>[QC]: Verify Size fail(C3)>DiskSize mismatch user setting
0xC4>[QC]: FW version mismatch(C4)>FW Version mismatch user setting
0xC5>[QC]: Vendor Specific mismatch(C5)>Vendor Specific mismatch user setting
0xC6>[QC]: WWN mismatch(C6)>WWN16 mismatch user setting
0xC7>[QC]: Read CID fail(C7)>Vendor Command flow fail at ReadCID
0xC8>[QC]: CID mismatch, See Log file(C8)>CID content mismatch MPTool input data
0xD3>Check Image fail (D3)>Check Image size or file system size error
0xE0>MPISP can't support Intel grade check (E0)>MPISP didn't support Intel Grade check function
0xE1>Special Grade (E1)>Find Special Intel Grade, Ex. (Chx,CeX=0x00)
0xED>Create partition fail (ED)>Create partition with MBR fail
0xEE>Clear SMART fail (EE)>Reset SMART fail
0xEF>Trim write fail (EF)>Write ATA Trim command fail
0xF0>Can't find any system block at ISP Mode (F0)>SWPtest.dll dump nothing  at ISP Mode
0xF1>B0kb Sorting function fail (F1)/(3F.01)>Vendor command flow fail when program block
0xF2>Mixed different B0kb Program flash (F2)>Mixed 2-8 and 4-8 program flash on the device
0xF3>Wrong package. This is 2-8/4-8 program B0kb flash (F3)>Use wrong package to initial card
0xF5>Change ID command fail (F5)>Vendor command flow fail
0xF7>Read Retry Table function fail (F7)/(40.01)>Vendor command flow fail when get new retry table
0xF7>Read Retry Table function fail (F7)/(40.02)>Not exist Retry Table
0xFA>Exceed two channel, this fw can't support (FA)>"LBiCS" fw version just support one or two channel
0xFB>Exceed 8 Way, this fw can't support (FB)>"BiCS" fw version just support <= 8-way interleave
