0x01>Open device handle fail (01)>無法取得裝置Handle
0x02>Allocate memory fail (02)>無法配置一些緩衝區來啟動開卡線程
0x07>Initial Parameter fail (07)>初始參數錯誤
0x08>Check FW RunMode fail (08)>供應商命令流程失敗當要取得目前FW跑在哪個模式下 
0x09>Read Parameter Table fail (09.01)>供應商命令流程失敗當要讀取參數表
0x09>Read Parameter Table fail (09.02)>找不到參數表內指定的字符串或標籤
0x09>Read Parameter Table fail (09.03)>找不到FlashID資訊
0x0A>Read IDTable fail (0A)>供應商命令流程失敗當要讀取 IDTable時
0x0B>Keep Serial number fail (0B)>無法從IDTable或MPInfo獲取序號
0x0C>Read MPInfo fail (0C)>供應商命令流程失敗當要讀取MPInfo時
0x0D>Check ChangeID flag fail (0D.01)>供應商命令流程失敗當要讀取參數表時
0x0D>Check ChangeID flag fail (0D.03)>參數表錯誤
0x0E>Read CID fail (0E)>讀取 CID 時遇到供應商命令流程失敗
0x0F>Compare Flash Fail (0F)>Flash名稱與FlashDB不符合
0x10>Download MPISP fail (10)>載入MPISP過程時遇到配置內存失敗
0x11>Download MPISP fail (11)/(04.02)>供應商命令流程失敗當要強制進入ROM Code模式時
0x11>Download MPISP fail (11)/(06.02)>供應商命令流程失敗當要載入代碼時
0x11>Download MPISP fail (11)/(06.03)>供應商命令流程失敗當要取得目前FW跑在哪個模式下
0x11>Download MPISP fail (11)/(06.04)>供應商命令流程失敗當要重置 CPU時
0x13>Read FlashID fail after download MPISP (13)>供應商命令流程失敗當要讀取FlashID時
0x14>Can't support this unbalanced configuration (14)>不支援不對稱配置
0x15>Can't support multi-die unbalanced mode (15)>不支援多疊Die不對稱配置
0x16>Can't support this multi-die unbalanced configuration (16)>現在只支援 缺的那顆NAND要是最後CE或最後的Die
0x17>Compare Flash Fail (17)>FlashID 資訊與FlashDB不符合
0x18>GPIO Check fail (18)/(3C.01)>檢查有關Toggle Pin 的設置
0x18>GPIO Check fail (18)/(3C.02)>檢查有關 Reliable Pin 的設置
0x18>GPIO Check fail (18)/(3C.03)>供應商命令流程失敗
0x18>GPIO Check fail (18)/(3C.04)>檢查有關 AleExtend Pin 的設置
0x19>Channel0-CE0 didn't exist flash (19)>不支援 CH0 & CE0 不存在的佈局
0x1A>Check MPISP Mode fail (1A)>供應商命令流程失敗
0x1B>Not MPISP Mode (1B)>目前不是MPISP模式
0x1C>Check SanDisk Bics Read Retry fail (1C)/(3B.01)>供應商命令流程失敗
0x1D>Some die didn't support RR function (1D)>有些 Die不支援 Read Retry功能
0x1E>Read B16/B17 Grade fail (1E)/(3A.01)>供應商命令流程失敗
0x1F>Flash Mixed Different Grade (1F)>混到不同等級的Flash
0x20>Dump system block fail (20)/(13.01)>載入參數表失敗
0x20>Dump system block fail (20)/(13.02)>讀取Flash Page時遇到供應商命令流程失敗
0x20>Dump system block fail (20)/(13.03)>讀取所有 INFO Block失敗
0x20>Dump system block fail (20)/(13.04)>讀取所有 ISP Block失敗
0x20>Dump system block fail (20)/(13.05)>讀取 Bad Info資訊發生ECC失敗
0x21>SRAM Test fail (21)/(07.01)>供應商命令流程失敗
0x21>SRAM Test fail (21)/(07.02)>SRAM測試失敗
0x22>Flash Connectivity Test fail (22)/(08.0A)>讀取FlashID時遇到供應商命令流程失敗
0x22>Flash Connectivity Test fail (22)/(08.0B)>讀Flash連接測試時遇到供應商命令流程失敗
0x22>Flash Connectivity Test fail (22)/(08.12)>FlashID 不同於 FlashDB 設置
0x23>Generate CH/CE Map fail (23)/(0E.01)>CH或CE的數量為零
0x23>Generate CH/CE Map fail (23)/(0E.0C)>每個 CE 的 Die 數量與DataBase不同
0x23>Generate CH/CE Map fail (23)/(0E.0D)>每個CH的CE位置是不同的
0x23>Generate CH/CE Map fail (23)/(0E.0E)>CE組態與設置不符合
0x23>Generate CH/CE Map fail (23)/(0E.0F)>CH組態與設置不符合
0x24>Build Parameter Table fail (24)/(12.27)>這不是TLC Flash 
0x24>Build Parameter Table fail (24)/(12.28)>檢查參數表的內容正確性失敗
0x25>Set CardMode fail (25)/(26.01)>供應商命令流程失敗
0x25>Set CardMode fail (25)/(26.02)>將L06B轉換為B0KB失敗
0x26>TranRTC fail (26)>供應商命令流程失敗 (Dll功能)
0x27>TranADJ fail (27)/(0C.01)>No Good Window 可讀取
0x27>TranADJ fail (27)/(0C.02)>No Good Window 可寫入
0x27>TranADJ fail (27)/(0C.03)>寫入全部失敗在TranRead (Dll功能)
0x27>TranADJ fail (27)/(0C.04)>讀取全部失敗在TranRead (Dll功能)
0x27>TranADJ fail (27)/(0C.05)>寫入全部失敗在TranProgram (Dll功能)
0x27>TranADJ fail (27)/(0C.06)>讀取全部失敗在TranProgram (Dll功能)
0x27>TranADJ fail (27)/(0C.07)>Tran 介面失敗
0x2A>Get LastTimeBad fail (2A)>緩衝區偏移量超出，可能是InfoBlock資訊錯誤
0x2B>Get RunTimeBad fail (2B.01)>TotalRunTimeBad 數量為零
0x2B>Get RunTimeBad fail (2B.02)>TotalRunTimeBad 數量太大
0x2B>Get RunTimeBad fail (2B.03)>FBlock 索引超出範圍
0x2D>Get LastTimeBad fail (2D)/(39.01)>InfoTotalBlkStatusAddr大小錯誤
0x2D>Get LastTimeBad fail (2D)/(39.02)>InfoTotalBlkFinalAddr大小錯誤
0x2E>Get RunTimeBad fail (2E)/(38.01)>PtestGetDumpRuntimeBadStatus失敗
0x2E>Get RunTimeBad fail (2E)/(38.02)>TotalRunTimeBadPtrCnt 超出
0x2E>Get RunTimeBad fail (2E)/(38.03)>BadInfoFBlkOffset 超出
0x2F>Shallow Erase check fail (2F)/(3D.01)>供應商命令流程失敗
0x2F>Mixed Shallow Erase (2F)/(3D.02)>樣品混料
0x2F>Shallow Erase check fail (2F)/(3D.03)>讀取參數頁面失敗在樣品未混料情況
0x2F>Mixed Shallow Erase (2F)/(3D.03)>讀取參數頁面失敗在可接受樣本混料的設定
0x30>Scan OriginalBad fail (30)/(30.01)>執行讀取CMD時發生Nand Flash超時
0x30>Scan OriginalBad fail (30)/(30.02)>Block位置溢位
0x30>Scan OriginalBad fail (30)/(30.03)>Block位置錯誤
0x30>Scan OriginalBad fail (30)/(30.04)>也許是SRAM問題，請檢查TSB SRAM！
0x30>Scan OriginalBad fail (30)/(30.05)>ScanBad模式設置錯誤
0x32>Sort EraseBad fail (32)/(32.01)>執行抹除 CMD時發生Nand Flash超時
0x32>Sort EraseBad fail (32)/(32.02)>Block位置溢位
0x32>Sort EraseBad fail (32)/(32.03)>Block位置錯誤
0x32>Sort EraseBad fail (32)/(32.04)>也許是SRAM問題，請檢查TSB SRAM！
0x32>Sort EraseBad fail (32)/(32.05)>寫入備份OrgBad資訊時遇到供應商命令流程失敗
0x32>Sort EraseBad fail (32)/(32.06)>寫入最後的SLC組態到SRAM發生錯誤
0x34>Program dummy fail (34)/(31.01)>寫 Dummy 命令時發生Nand Flash 超時
0x34>Program dummy fail (34)/(31.02)>Block位置溢位
0x34>Program dummy fail (34)/(31.03)>Block位置錯誤
0x34>Program dummy fail (34)/(31.04)>也許是SRAM問題，請檢查TSB SRAM！
0x34>Program dummy fail (34)/(31.05)>寫入備份OrgBad資訊時遇到供應商命令流程失敗
0x34>Program dummy fail (34)/(31.06)>寫入最後的SLC組態到SRAM發生錯誤
0x40>Set System & Boundary Block fail (40)/(23.01)>系統區塊資訊超出範圍
0x40>Set System & Boundary Block fail (40)/(23.02)>第一個區塊 (Block)是不同
0x40>Set System & Boundary Block fail (40)/(23.03)>找不到足夠多好的 Block來存系統區塊資訊
0x41>Generate DiffAddr Table fail (41)/(0F.01)>構建SLC Diff Addr表失敗
0x41>Generate DiffAddr Table fail (41)/(0F.02)>構建TLC Diff Addr表失敗
0x41>Generate DiffAddr Table fail (41)/(0F.03)>選擇不符合失敗
0x41>Generate DiffAddr Table fail (41)/(0F.04)>Later Bad 數量計算失敗
0x41>Generate DiffAddr Table fail (41)/(0F.05)>在TLC範圍內有最後一個SLC Block
0x41>Generate DiffAddr Table fail (41)/(0F.06)>在SLC範圍內的第一個TLC Block
0x41>Generate DiffAddr Table fail (41)/(0F.07)>擴展 8K的 Diff Table 超出範圍
0x41>Generate DiffAddr Table fail (41)/(0F.09)>發現重疊 DIFF 位置
0x41>Generate DiffAddr Table fail (41)/(0F.0A)>Physical區塊位置超過 Super區塊位置
0x42>Set Disk Capacity fail (42)/(0D.01)>手動設置容量超出失敗
0x42>Set Disk Capacity fail (42)/(0D.15)>SLC Block 不足
0x42>Set Disk Capacity fail (42)/(0D.16)>壞塊過多 !!
0x43>Calculate Info Block length fail (43)/(10.19)>在計算 BootISP占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.20)>在計算 Seed Table 占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.21)>在計算 Parameter Table 占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.22)>在計算 BadBlockStatus Table 占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.23)>在計算 BadBlockBitMap占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.24)>在計算 DiffType2Bit占的大小時失敗 (大小會對齊Plane數)
0x43>Calculate Info Block length fail (43)/(10.25)>在計算 TotalDiffAddr占的大小時失敗 (大小會對齊Plane數)
0x44>Compare Flash Fail (44)>Flash資訊不符
0x45>Check Program Time Fail (45)>Pretest模式不支援測速
0x46>Check Max RDT Temperature (46)>低於最大RDT溫度
0x47>Check RDT Version (47)>RDT版本不批配
0x48>Check Device Status Fail (48)>裝置狀態不支援此Pretest模式
0x4A>Generate InfoBlk fail (4A)>DLL 回覆 INFO區塊資訊長度為零
0x4B>Generate InfoBlk fail (4B)>在生成 INFO 區塊資訊過程時發生配置內存失敗
0x4C>Generate InfoBlk fail (4C)/(10.19)>在計算 BootISP占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.20)>在計算 Seed Table 占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.21)>在計算 Parameter Table 占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.22)>在計算 BadBlockStatus Table 占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.23)>在計算 BadBlockBitMap占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.24)>在計算 DiffType2Bit占的大小時失敗 (大小會對齊Plane數)
0x4C>Generate InfoBlk fail (4C)/(10.25)>在計算 TotalDiffAddr占的大小時失敗 (大小會對齊Plane數)
0x4D>Generate InfoBlk fail (4D)/(11.26)>參數表不存在
0x4E>Generate InfoBlk fail (4E)/(24.01)>抹除 INFO區塊資訊時遇到供應商命令流程失敗
0x4E>Generate InfoBlk fail (4E)/(24.02)>寫入INFO區塊資訊時遇到供應商命令流程失敗
0x4E>Generate InfoBlk fail (4E)/(24.03)>抹除 Index 區塊時遇到供應商命令流程失敗
0x4E>Generate InfoBlk fail (4E)/(24.04)>寫入 Index 區塊時遇到供應商命令流程失敗
0x4F>Verify InfoBlk fail (4F)/(24.05)>計算的校驗和 (Checksum) 與從 Nand Flash讀到的校驗和不同
0x4F>Verify InfoBlk fail (4F)/(24.06)>讀取INFO區塊資訊時出現ECC失敗
0x4F>Verify InfoBlk fail (4F)/(24.07)>讀取INFO區塊資訊時遇到供應商命令流程失敗
0x50>Erase System block fail (50)>無法轉換 Physical 的系統區塊索引
0x51>Erase System block fail (51)>抹除系統區塊時遇到供應商命令流程失敗
0x54>Bin Level not found fail (54)>找不到Bin級
0x55>Table not found fail (55)>找不到Block ECC Table
0x60>Download ISP fail (60)>載入ISP程序時發生配置內存失敗
0x61>Download ISP fail (61)/(25.01)>抹除ISP時遇到供應商命令流程失敗
0x61>Download ISP fail (61)/(25.02)>寫入ISP時遇到供應商命令流程失敗
0x61>Download ISP fail (61)/(25.03)>計算校驗和 (Checksum)過程發生錯誤
0x62>Verify ISP fail (62)/(22.01)>計算的校驗和 (Checksum) 與從Nand Flash讀取的校驗和不同
0x62>Verify ISP fail (62)/(22.02)>讀取ISP區塊時發生 ECC失敗
0x62>Verify ISP fail (62)/(22.03)>檢查ISP校驗和時遇到供應商命令流程失敗
0x63>Verify ISP fail (63.01)>將參數表寫入SRAM時遇到供應商命令流程失敗
0x63>Verify ISP fail (63)/(13.01)>載入參數表失敗
0x63>Verify ISP fail (63)/(13.02)>讀取Flash Page時遇到供應商命令流程失敗
0x63>Verify ISP fail (63)/(13.03)>讀取所有 INFO區塊失敗
0x63>Verify ISP fail (63)/(13.04)>讀取所有 ISP 區塊失敗
0x63>Verify ISP fail (63)/(13.05)>讀取BadInfo區塊發生ECC失敗
0x63>Verify ISP fail (63.02)>比較 ISP 內容不正確
0x6A>Download MPInfo fail (6A)/(21.01)>抹除MPInfo區塊時遇到供應商命令流程失敗
0x6A>Download MPInfo fail (6A)/(21.02)>寫入MPInfo區塊時遇到供應商命令流程失敗
0x70>Reset Drive fail (70)/(04.04)>重置CPU時到供應商命令流程失敗
0x7A>Check ISP Mode fail (7A)>供應商命令流程失敗
0x7B>Not ISP Mode (7B)>在下CPU重置後發現沒有進入ISP模式
0x80>Read Drive Info fail (80)/(0B.01)>讀取裝置資訊時遇到供應商命令流程失敗
0x81>Get Firmware Version fail (81)>讀取IDTable時遇到供應商命令流程失敗
0xA0>Read RDT Result fail (A0)>讀取 RDT 結果過程時遇到配置內存失敗
0xA1>Read RDT Result fail (A1)/(35.01)>Seed Table 錯誤
0xA1>Read RDT Result fail (A1)/(35.02)>找不到 RDT 區塊
0xA1>Read RDT Result fail (A1)/(35.03)>讀取RDT結果時遇到供應商命令流程失敗
0xA1>Read RDT Result fail (A1)/(35.04)>讀取RAM失敗在 Step1
0xA1>Read RDT Result fail (A1)/(35.05)>讀取RAM失敗在 Step2
0xA1>Read RDT Result fail (A1)/(35.06)>讀取RAM失敗在 Step3
0xA1>Read RDT Result fail (A1)/(35.07)>讀取RAM失敗在 Step4
0xA1>Read RDT Result fail (A1)/(35.08)>RDT結果不正確 
0xA1>Read RDT Result fail (A1)/(35.09)>RDT超時
0xA2>RDT Result is not exist (A2)>無法從RDT結果緩衝區中找到 RDT@ 字符串
0xA3>RDT is unfinished (A3)>RDT未完成因 RDT_PASS 標誌為零
0xA4>RDT Result is FAIL (A4)>RDT結果失敗因RDT_ErrorCode有值
0xA5>Check Max RDT ECC TH (A5)>超過最大RDT ECC臨界值
0xA6>Pre-Check Capacity fail (A6)/(0F.01)>構建SLC Diff Addr表失敗
0xA6>Pre-Check Capacity fail (A6)/(0F.02)>構建TLC Diff Addr表失敗
0xA6>Pre-Check Capacity fail (A6)/(0F.03)>選擇不符合失敗
0xA6>Pre-Check Capacity fail (A6)/(0F.04)>Later Bad 數量計算失敗
0xA6>Pre-Check Capacity fail (A6)/(0F.05)>在TLC範圍內有最後一個SLC Block
0xA6>Pre-Check Capacity fail (A6)/(0F.06)>在SLC範圍內的第一個TLC Block
0xA6>Pre-Check Capacity fail (A6)/(0F.07)>擴展 8K的 Diff Table 超出範圍
0xA6>Pre-Check Capacity fail (A6)/(0D.01)>手動容量超出失敗
0xA6>Pre-Check Capacity fail (A6)/(0D.15)>SLC Block不足
0xA6>Pre-Check Capacity fail (A6)/(0D.16)>壞快過多 !!
0xB0>Copy Test fail (B0)>在CopyCompare程序之前檢查出不是ISP模式
0xB1>Copy Test fail (B1)>在CopyCompare過程中出現配置內存失敗
0xB2>Copy Test fail (B2)>在CopyCompare過程中出現配置內存失敗 (為了存自訂的資料樣本)
0xB3>Copy Test fail (B3)>在CopyCompare過程中出現讀取自訂的資料樣本失敗
0xB4>Copy Test fail (B4)>在CopyCompare過程中出現配置內存失敗 (生成隨機的資料樣本))
0xB5>Copy Test (write) fail (B5)>在CopyCompare過程中出現寫入失敗
0xB6>Copy Test (read) fail (B6)>在CopyCompare過程中出現讀取失敗
0xB7>Copy Test (compare) fail (B7)>在CopyCompare過程中出現比較數據失敗
0xB8>Copy Test (clean) fail (B8)>在CopyCompare過程中出現清除數據失敗
0xC0>[QC]: It's not ISP Mode(C0)>在執行QC程序之前檢查出不是ISP模式
0xC1>[QC]: Read IDTable/MPInfo fail(C1)>讀 IDTable和 MPInfo中的遇到供應商命令流程失敗
0xC2>[QC]: MPInfo mismatch, See Log file(C2)>MPInfo（SN + ModelName + WWN8）不同於使用者設置
0xC3>[QC]: Verify Size fail(C3)>磁碟類型不同於使用者設置
0xC4>[QC]: FW version mismatch(C4)>韌體版本不同於使用者設置
0xC5>[QC]: Vendor Specific mismatch(C5)>廠商名稱不同於使用者設置
0xC6>[QC]: WWN mismatch(C6)>WWN16不符合使用者設置
0xC7>[QC]: Read CID fail(C7)>讀取 CID 時遇到供應商命令流程失敗
0xC8>[QC]: CID mismatch, See Log file(C8)>CID內容不同於MPTool輸入資訊
0xD3>Check Image fail (D3)>映像檔或檔案系統大小錯誤
0xE0>MPISP can't support Intel grade check (E0)>MPISP不支援 Intel Grade 檢查功能
0xE1>Special Grade (E1)>找尋特殊 Intel Grade, 例如（CHx，CEx = 0x00）
0xEC>Delete partition fail (EC)>刪除分區失敗
0xED>Create partition fail (ED)>建立 MBR 分區失敗
0xEE>Clear SMART fail (EE)>重置 SMART 失敗
0xEF>Trim write fail (EF)>寫入 ATA Trim 命令失敗
0xF0>Can't find any system block at ISP Mode (F0)>在ISP模式下但找不到任何 System 區塊
0xF1>B0kb Sorting function fail (F1)/(3F.01)>寫入區塊時遇到供應商命令流程失敗
0xF2>Mixed different B0kb Program flash (F2)>B0KB 混料 (裡面有混2-8和4-8 Program Order 的組合) 
0xF3>Wrong package. This is 2-8/4-8 program B0kb flash (F3)>使用錯誤的開卡包
0xF5>Change ID command fail (F5)>供應商命令流程失敗
0xF7>Read Retry Table function fail (F7)/(40.01)>讀取新的 Retry Table 時遇到供應商命令流程失敗
0xF7>Read Retry Table function fail (F7)/(40.02)>Retry Table 不存在
0xFA>Exceed two channel, this fw can't support (FA)>LBiCS FW 版只支援一個或兩個 Channel 
0xFB>Exceed 8 Way, this fw can't support (FB)>BiCS FW版本只支援小於或等於 8-Way Interleave 
0xFD>Database Plane mode is different to device's plane mode>請使用 Don't Ref. Original Bad 或 Force Plane mode
