

;================================================================================
{SetMsgColor = BLUE}
 80 00, "      GC        (%0Ad ms), GC state: 0x%04X ", 4 2
 80 01, "      GC        (%0Ad ms), GC flow: 0x%04X ", 4 2
 80 02, "      GC        (%0Ad ms), zero VPC source block: 0x%04X ", 4 2
 80 03, "      GC        (%0Ad ms), GC source block cnt: 0x%04X ", 4 2
 80 04, "      GC        (%0Ad ms), GC source block: 0x%04X ", 4 2
 80 05, "      GC        (%0Ad ms), GC source VPC: 0x%08X ", 4 4
 80 06, "      GC        (%0Ad ms), GC des block: 0x%04X ", 4 2
 80 07, "      GC        (%0Ad ms), Static mode: 0x%04X ", 4 2
 80 08, "      GC        (%0Ad ms), SLC spare block count: 0x%04X ", 4 2
 80 09, "      GC        (%0Ad ms), TLC full cache block count: 0x%04X ", 4 2


;================================================================================
{SetMsgColor = GREEN}
 81 00, "      FTL       (%0Ad ms), FlushF2hStr=0x%04X,End=0x%04X ,HBlkNum=0x%04X", 4 2 2 2


;================================================================================
{SetMsgColor = BLACK}
 83 00, "      BuildLink (%0Ad ms),  rdlinkFunc() ", 4
 83 01, "      BuildLink (%0Ad ms),  Build Link Finish! ", 4
 83 02, "      BuildLink (%0Ad ms),  Save Event Log ", 4
 83 03, "      BuildLink (%0Ad ms),  Boot from Qboot", 4
 83 04, "      BuildLink (%0Ad ms),  Boot need Rebuild", 4
 83 05, "      BuildLink (%0Ad ms), Spare cnt: 0x%04X ", 4 2
 83 06, "      BuildLink (%0Ad ms), TLC spare cnt: 0x%04X ", 4 2
 83 07, "      BuildLink (%0Ad ms), GC type bit: 0x%04X ", 4 2
 83 08, "      BuildLink (%0Ad ms), GC Queue cnt: 0x%04X ", 4 2
 83 09, "      BuildLink (%0Ad ms), Spare cnt: 0x%04X, TLC spare cnt: 0x%04X, GC type bit: 0x%04X, GC Queue cnt: 0x%04X", 4 2 2 2 2
 83 0A, "      BuildLink (%0Ad ms),  ChkEmptyPgSpr:[0x%04X, 0x%04X], [0x%04X, 0x%04X, 0x%04X, 0x%04X] ", 4 2 2 2 2 2 2


;================================================================================
{SetMsgColor = PURPLE}
 84 06, "      Host      (%0Ad ms),  FW commit-Action Error, Action=0x%04X ", 4 2
 84 07, "      Host      (%0Ad ms),  FW commit-Slot Error, Slot=0x%04X ", 4 2
 84 08, "      Host      (%0Ad ms),  FW Image Download - No transfer data, NUMD=0x%08X ", 4 4
 84 09, "      Host      (%0Ad ms),  FW Image Download - PRP Error ", 4
 84 0A, "      Host      (%0Ad ms),  FW Image Download - Overlapping Range ", 4
 84 0B, "      Host      (%0Ad ms),  VDT18 Fail(ISR) ", 4
 84 0C, "      Host      (%0Ad ms),  VDT23 Fail(ISR) ", 4
 84 0D, "      Host      (%0Ad ms),  VDT27 Fail(ISR) ", 4
 84 0E, "      Host      (%0Ad ms),  FWRQ_RDY(ISR) ", 4
 84 0F, "      Host      (%0Ad ms),  Doorbell(ISR) ", 4
 84 10, "      Host      (%0Ad ms),  NVMe NSSR(ISR), Link State=0x%04X ", 4 2
 84 11, "      Host      (%0Ad ms),  NVMe Reset(ISR), Link State=0x%04X ", 4 2
 84 12, "      Host      (%0Ad ms),  NVMe EN (cc_en on)(ISR), Link State=0x%04X ", 4 2
 84 13, "      Host      (%0Ad ms),  PCIe Funcrion Level RST(ISR), Link State=0x%04X ", 4 2
 84 14, "      Host      (%0Ad ms),  NVMe Shut Down Notification(ISR), Link State=0x%04X ", 4 2
 84 15, "      Host      (%0Ad ms),  NVMe Shut Down Notification(ISR), Link State=0x04X ", 4
 84 16, "      Host      (%0Ad ms), PCIe Link down(ISR) , Link State=0x%04X ", 4 2
 84 17, "      Host      (%0Ad ms),  CPL time out(ISR), Link State=0x%04X ", 4 2
 84 18, "      Host      (%0Ad ms),  LTSSM_Trace0(ISR), Link Stare=0x%04X ", 4 2
 84 19, "      Host      (%0Ad ms),  LTSSM_Trace1(ISR), Link State=0x%04X ", 4 2
 84 1A, "      Host      (%0Ad ms),  Malform TLP(ISR), log0=0x%08X, log1=0x%08X ", 4 4 4
 84 1B, "      Host      (%0Ad ms),  Malform TLP(ISR), log2=0x%08X, log3=0x%08X ", 4 4 4
 84 1C, "      Host      (%0Ad ms),  Malform TLP(ISR), Link State=0x%04X ", 4 2
 84 1D, "      Host      (%0Ad ms),  DHY src0(ISR), Link State=0x%04X ", 4 2
 84 1E, "      Host      (%0Ad ms),  DHY src1(ISR), Link State=0x%04X ", 4 2
 84 1F, "      Host      (%0Ad ms),  DHY src2(ISR), Link State=0x%04X ", 4 2
 84 20, "      Host      (%0Ad ms),  DPHY src3(ISR), Link State=0x%04X ", 4 2
 84 21, "      Host      (%0Ad ms),  Set Feature ID=0x%04X, SV=0x%04X, Attr=0x%08X", 4 2 2 4
 84 22, "      Host      (%0Ad ms),  NVMe Device Selt-test Command Received, Selt-Test Code=0x%04X ", 4 2
 84 23, "      Host      (%0Ad ms),  NVMe Device Selt-test Start time at %08d ms ", 4 4
 84 24, "      Host      (%0Ad ms),  NVMe Device Selt-Test Abort, Current DST Operation=0x%04X ", 4 2
 84 25, "      Host      (%0Ad ms),  NVMe Device Self-test Processing Segment=0x%04X ", 4 2
 84 26, "      Host      (%0Ad ms),  NVMe Device Self-test Completed,  FailSegmentBitMap=0x%04X,  DSTPeriod=%08d ms ", 4 2 4
 84 27, "      Host      (%0Ad ms),  VDT 2.7 Fail (ISR) ", 4
 84 28, "      Host      (%0Ad ms),  VDT 4.0 Fail WDT (ISR)", 4
 84 29, "      Host      (%0Ad ms),  PCIe Reset P11(ISR), Link State=0x%04X ", 4 2
 84 2A, "      Host      (%0Ad ms),  VDT FIO 1.2V Fail(ISR) ", 4
 84 2B, "      Host      (%0Ad ms),  ISR16-Other(ISR) ", 4
 84 2C, "      Host      (%0Ad ms),  Dx to D0 (ISR), Link State=0x%04X ", 4 2
 84 2D, "      Host      (%0Ad ms),  D0 to Dx=0x%04X (ISR), Link State=0x%04X ", 4 2 2
 84 2E, "      Host      (%0Ad ms),  Get FID=0x%04X, SEL=0x%04X ", 4 2 2
 84 2F, "      Host      (%0Ad ms), PCIe Init, Link State=0x%04X ", 4 2
 84 30, "      Host      (%0Ad ms),  resetNvmeIp(), Invalid write DB, bitmap=0x%08X ", 4 4
 84 31, "      Host      (%0Ad ms),  resetNvmeIp(), Write Empty=%04d, Read Empty=%04d ", 4 2 2
 84 32, "      Host      (%0Ad ms),  NVMe Reset done, Link State=0x%04X ", 4 2
 84 33, "      Host      (%0Ad ms),  Shutdown complete, Link State=0x%04X ", 4 2
 84 34, "      Host      (%0Ad ms),  NVMe EN (set cc_rdy),  Link State=0x%04X ", 4 2
 84 35, "      Host      (%0Ad ms),  PRP Error, uCmdType = 0x%04X, uError = 0x%04X ", 4 2 2
 84 36, "      Host      (%0Ad ms),  PRP1 HiDWORD=0x%08X,  LoDWORD=0x%08X ", 4 4 4
 84 37, "      Host      (%0Ad ms),  PRP2 HiDWORD=0x%08X,  LoDWORD=0x%08X ", 4 4 4
 84 38, "      Host      (%0Ad ms),  NVMe Flush Cmd ", 4
 84 39, "      Host      (%0Ad ms),  PCIe Function Level RST(ISR), Link State=0x%04X ", 4 2
 84 3A, "      Host      (%0Ad ms),  PHY Setting readback error, Addr=0x%04X, ExpVal=0x%02X, ActVal=0x%02X ", 4 2 1 1
 84 3B, "      Host      (%0Ad ms),  CPL TO Stop Fetch CMD, ChkBridgeAxiRwFlushBsy=0x%04X ", 4 2
 84 3C, "      Host      (%0Ad ms),  PRD PDTR0=0x%04X ", 4 2
 84 3D, "      Host      (%0Ad ms),  PRD PDTR1=0x%04X ", 4 2
 84 3E, "      Host      (%0Ad ms),  Host ShutDown notification", 4
 84 3F, "      Host      (%0Ad ms),  Host Shutdown notification End ", 4
 84 40, "      Host      (%0Ad ms),   APST Entery :0x%04X, Power State: 0x%04X,  Idle Time: 0x%08X", 4 2 2 4
 84 41, "      Host      (%0Ad ms),  NVMe SHN Change 1->0 Clr Interrput(ISR), Link State=0x04X ", 4
 84 42, "      Host      (%0Ad ms),  HMB MR=0 and HMB invalid !!", 4
 84 43, "      Host      (%0Ad ms),  HMB MR=1 and HMB invalid !!", 4
 84 44, "      Host      (%0Ad ms),  Hmb Enable Fail, HSIZE<MHMMIN.", 4
 84 45, "      Host      (%0Ad ms),  Hmb Enable Fail, Descriptor Entry Memory OverLapping.", 4
 84 46, "      Host      (%0Ad ms),  Hmb Enable Fail, Hmb not enough within 256 entry.", 4
 84 47, "      Host      (%0Ad ms),  Hmb Enable success", 4


;================================================================================
{SetMsgColor = OLIVE}
 85 00, "      PS        (%0Ad ms),  L1 time out, CLKREQ-Deassert ", 4
 85 01, "      PS        (%0Ad ms),  L1 time out, CLKREQ-Assert ", 4
 85 02, "      PS        (%0Ad ms),  L1 time out ", 4
 85 03, "      PS        (%0Ad ms),  Host set feature - Power state=0x%02X, CurPS=0x%02X ", 4 1 1
 85 04, "      PS        (%0Ad ms),  chkHostIdle busy: NVMe Idle Bitmap=0x%04X ", 4 2
 85 05, "      PS        (%0Ad ms),   chkHostIdle busy: Get new cmd ", 4
 85 06, "      PS        (%0Ad ms),  Host set feature - Power state=0x%04X, CurPS=0x%04X ", 4 2 2
 85 07, "      PS        (%0Ad ms),  CQ busy: QID=0x%04X, HeadDB=0x%04X, TailDB=0x%04X ", 4 2 2 2
 85 08, "      PS        (%0Ad ms),  SQ busy: QID=0x%04X, TailDB=0x%04X, HeadDB=0x%04X ", 4 2 2 2
 85 09, "      PS        (%0Ad ms),  busy: sq_cmd_buf ", 4
 85 0A, "      PS        (%0Ad ms),  busy: hwcq ", 4
 85 0B, "      PS        (%0Ad ms),  busy: dmacq ", 4
 85 0C, "      PS        (%0Ad ms),  busy: fwcq ", 4
 85 0D, "      PS        (%0Ad ms),  busy: fwrq ", 4
 85 0E, "      PS        (%0Ad ms),  busy: prd ", 4
 85 0F, "      PS        (%0Ad ms),  busy: unex_engine ", 4
 85 10, "      PS        (%0Ad ms),  chkHostIdle busy: NVMe reset ", 4
 85 11, "      PS        (%0Ad ms),  chkHostIdle busy: NVMe shutdown ", 4
 85 12, "      PS        (%0Ad ms),  chkHostIdle busy: PCIe link down ", 4
 85 13, "      PS        (%0Ad ms),  chkHostIdle busy: PCIe reset-P11", 4
 85 14, "      PS        (%0Ad ms),  Assert ClkReq(ISR) ", 4
 85 15, "      PS        (%0Ad ms),  hdlHipmProc(), Try to enter L1.2 ", 4
 85 16, "      PS        (%0Ad ms),  Deassert=0x%04X, EnL1=0x%04X, EnL0s=0x%04X ", 4 2 2 2
 85 17, "      PS        (%0Ad ms),  ClkPS, Support=0x%04X, Enable=0x%04X ", 4 2 2
 85 18, "      PS        (%0Ad ms),  ASPML11, Support=0x%04X, Enable=0x%04X ", 4 2 2
 85 19, "      PS        (%0Ad ms),  ASPML12, Support=0x%04X, Enable=0x%04X ", 4 2 2
 85 1A, "      PS        (%0Ad ms), hdlHipmProc(), Host En L11&L12=0x%04X", 4 2
 85 1B, "      PS        (%0Ad ms),  BootFunc(), PS0 completion. ", 4
 85 1C, "      PS        (%0Ad ms),  Boot from NVMe PS4, Device CurState=%04d, CC_EN=0x%02X, CC_RDY=0x%02X, CMD_RDY=0x%04X ", 4 2 1 1 2
 85 1D, "      PS        (%0Ad ms),  PS4 resume, PCIe Init_0_1_Sts=0x%08X, PCIe Int_2_3_Sts=0x%08X ", 4 4 4
 85 1E, "      PS        (%0Ad ms),  PS4 resume, NVMe Init_LOW_Sts=0x%08X, PCIe Int_HIGH_Sts=0x%08X ", 4 4 4
 85 1F, "      PS        (%0Ad ms),  Boot from power off ", 4
 85 20, "      PS        (%0Ad ms),  idleBgTime=0x%08Xms, Host idle=0x%04X ", 4 4 2
 85 21, "      PS        (%0Ad ms),  NVMe PS4 Shutdown Proc Start ", 4
 85 22, "      PS        (%0Ad ms),  APST From PS0x%04X to PS0x%04X, idle time=0x%08X ms ", 4 2 2 4
 85 23, "      PS        (%0Ad ms),  Boot from power off 0x%04X", 4 2
 85 24, "      PS        (%0Ad ms), hdlHipmProc(), Host En L11&L12=0x%04X, PsChg=0x%04X", 4 2 2
 85 25, "      PS        (%0Ad ms), goto setSuspendMo(), Next PS=%04d", 4 2


;================================================================================
{SetMsgColor = MAROON}
 87 00, "      Admin     (%0Ad ms),  Admin Cmd OpCode=0x%04X ", 4 2


;================================================================================
{SetMsgColor = NAVY}
 88 00, "      ASSERT HANG (%0Ad ms),  Uart trigger save log ", 4
 88 01, "      ASSERT HANG (%0Ad ms),  PCIE_AXI_W_TIMEOUT ", 4
 88 02, "      ASSERT HANG (%0Ad ms),  PCIE_AXI_R_TIMEOUT ", 4
 88 03, "      ASSERT HANG (%0Ad ms),  AES2TSB_W_TIMEOUT ", 4
 88 04, "      ASSERT HANG (%0Ad ms),  AES2TSB_R_DRAM_TIMEOUT ", 4
 88 05, "      ASSERT HANG (%0Ad ms),  AES2TSB_R_SRAM_TIMEOUT ", 4
 88 06, "      ASSERT HANG (%0Ad ms), ARM error handlerr IFAR: 0x%08X ", 4 4
 88 07, "      ASSERT HANG (%0Ad ms), ARM error handlerr IFSR: 0x%08X ", 4 4
 88 08, "      ASSERT HANG (%0Ad ms), ARM error handlerr 1 bit error cpu status: 0x%04X ", 4 2
 88 09, "      ASSERT HANG (%0Ad ms), ARM error handlerr 2 bits error cpu status: 0x%04X ", 4 2
 88 0A, "      ASSERT HANG (%0Ad ms), ARM error handlerr DFAR: 0x%08X ", 4 4
 88 0B, "      ASSERT HANG (%0Ad ms), ARM error handlerr DFSR: 0x%08X ", 4 4
 88 0C, "      ASSERT HANG (%0Ad ms),  NVMe DMA error, DMA error bitmap=0x%04X ", 4 2
 88 0D, "      ASSERT HANG (%0Ad ms),  DMA Status [0]=0x%08X, [1]=0x%08X ", 4 4 4
 88 0E, "      ASSERT HANG (%0Ad ms),  DMA Status [2]=0x%08X, [3]=0x%08X ", 4 4 4
 88 0F, "      ASSERT HANG (%0Ad ms),  DMA Status [4]=0x%08X, [5]=0x%08X ", 4 4 4
 88 10, "      ASSERT HANG (%0Ad ms),  DMA Status [6]=0x%08X, [7]=0x%08X ", 4 4 4
 88 11, "      ASSERT HANG (%0Ad ms),  TSB_Bus_TIMEOUT(PCIE OR LDPC), Address = 0x%08X, Package Length = 0x%04X, Source = 0x%04X ", 4 4 2 2
 88 12, "      ASSERT HANG (%0Ad ms),  BVAC_Bus_TIMEOUT, Address = 0x%08X, Package Length = 0x%04X, Source = 0x%04X ", 4 4 2 2
 88 13, "      ASSERT HANG (%0Ad ms),  TSB_Bus_TIMEOUT(FLASH), Address = 0x%08X, Package Length = 0x%04X, Source = 0x%04X ", 4 4 2 2
 88 14, "      ASSERT HANG (%0Ad ms),  CPU_Bus_TIMEOUT, Address = 0x%08X ", 4 4
 88 15, "      ASSERT HANG (%0Ad ms),  VDT Fsh1 2.3V Fail ", 4
 88 16, "      ASSERT HANG (%0Ad ms),  VDT Fsh2 2.7V Fail ", 4
 88 17, "      ASSERT HANG (%0Ad ms),  VDT FIO 1.2V Fail ", 4
 88 18, "      ASSERT HANG (%0Ad ms), TSB ECC 2-bit uncorrectable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 19, "      ASSERT HANG (%0Ad ms), TSB ECC RMW 2-bit uncorrectable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 1A, "      ASSERT HANG (%0Ad ms), TSB4 ECC 2-bit uncorrectable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 1B, "      ASSERT HANG (%0Ad ms), TSB4 ECC RMW 2-bit uncorrectable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 1C, "      ASSERT HANG (%0Ad ms), TSB ECC RMW 1-bit correctable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 1D, "      ASSERT HANG (%0Ad ms), Error Bitmap=0x%08x%08x", 4 4 4
 88 1E, "      ASSERT HANG (%0Ad ms), TSB ECC 1-bit correctable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 1F, "      ASSERT HANG (%0Ad ms), TSB4 ECC RMW 1-bit correctable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 20, "      ASSERT HANG (%0Ad ms), TSB4 ECC 1-bit correctable error, Info=0x%08x, Addr(8byte align)=0x%08x", 4 4 4
 88 21, "      ASSERT HANG (%0Ad ms), ARM error handler IFAR: 0x%08X ", 4 4
 88 22, "      ASSERT HANG (%0Ad ms), ARM error handler IFSR: 0x%08X ", 4 4
 88 23, "      ASSERT HANG (%0Ad ms), ARM error handler 1 bit error cpu status: 0x%04X ", 4 2
 88 24, "      ASSERT HANG (%0Ad ms), ARM error handler 2 bits error cpu status: 0x%04X ", 4 2
 88 25, "      ASSERT HANG (%0Ad ms), ARM error handler DFAR: 0x%08X ", 4 4
 88 26, "      ASSERT HANG (%0Ad ms), ARM error handler DFSR: 0x%08X ", 4 4
 88 27, "      ASSERT HANG (%0Ad ms), E2E : User Data happened CRC error, Prd:0x%02X, Addr:0x%04X, Len:0x%04X, E2E Addr:0x%04X, E2E CRC:0x%04X", 4 1 2 2 2 2
 88 28, "      ASSERT HANG (%0Ad ms), ARM error handlerr IFSR: 0x%08X, 1 bit error cpu status: 0x%04X, 2 bits error cpu status: 0x%04X", 4 4 2 2
 88 29, "      ASSERT HANG (%0Ad ms), ARM error handlerr DFSR: 0x%08X, 1 bit error cpu status: 0x%04X, 2 bits error cpu status: 0x%04X", 4 4 2 2
 88 2A, "      ASSERT HANG (%0Ad ms), E2E : User Data happened CRC error, Prd:0x%04X, Addr:0x%08X, Len:0x%08X, E2E Addr:0x%08X", 4 2 4 4 4


;================================================================================
{SetMsgColor = TEAL}
 8A 00, "      Thermal/PS (%0Ad ms),  Standby Mode Entry ", 4
 8A 01, "      Thermal/PS (%0Ad ms),  PS3 State resume ", 4
 8A 02, "      Thermal/PS (%0Ad ms),  PS4 State resume ", 4
 8A 03, "      Thermal/PS (%0Ad ms),  Standby Mode resume ", 4
 8A 04, "      Thermal/PS (%0Ad ms),  Sensor0 output ", 4
 8A 05, "      Thermal/PS (%0Ad ms),  Sensor1 output ", 4
 8A 06, "      Thermal/PS (%0Ad ms),  NormalizationTemperature ", 4
 8A 07, "      Thermal/PS (%0Ad ms),  Not need Normalization ", 4
 8A 08, "      Thermal/PS (%0Ad ms),  PS3 State resume, CurPs=%02d, Wake Isr=%02d", 4 1 1
 8A 09, "      Thermal/PS (%0Ad ms),  Standby Mode resume, CurPs=%02d, Wake Isr=%02d", 4 1 1
 8A 0A, "      Thermal/PS (%0Ad ms),  PS4 State abort, CurPs=%02d, Wake Isr=%02d", 4 1 1
 8A 0B, "      Thermal/PS (%0Ad ms),  Sensor0 output=%04d ", 4 2
 8A 0C, "      Thermal/PS (%0Ad ms),  Sensor1 output=%04d ", 4 2
 8A 0D, "      Thermal/PS (%0Ad ms),  NormalizationTemperature=%04d ", 4 2


;================================================================================
{SetMsgColor = NAVY}
 8B 00, "      SYS       (%0Ad ms),  AER_SMART Temp Over, TH=0x%04X, Val=0x%04X ", 4 2 2
 8B 01, "      SYS       (%0Ad ms), ASSERT LOG: AER_SMART Read Only ", 4
 8B 02, "      SYS       (%0Ad ms),  ASSERT LOG: AER_SMART Mem Fail ", 4
 8B 03, "      SYS       (%0Ad ms),  NVMe DMA error, DMA error bitmap=0x%04X ", 4 2
 8B 04, "      SYS       (%0Ad ms),  DMA Status [0]=0x%08X, [1]=0x%08X ", 4 4 4
 8B 05, "      SYS       (%0Ad ms),  DMA Status [2]=0x%08X, [3]=0x%08X ", 4 4 4
 8B 06, "      SYS       (%0Ad ms),  DMA Status [4]=0x%08X, [5]=0x%08X ", 4 4 4
 8B 07, "      SYS       (%0Ad ms),  DMA Status [6]=0x%08X, [7]=0x%08X ", 4 4 4
 8B 08, "      SYS       (%0Ad ms),  AES Current LBA 0x%08X ", 4 4
 8B 09, "      SYS       (%0Ad ms),  UART trigger save log ", 4
 8B 0A, "      SYS       (%0Ad ms),  Invalid Doorbell, CQ bitmap=0x%04X, SQ bitmap=0x%04X ", 4 2 2
 8B 0B, "      SYS       (%0Ad ms),  E2E Current LBA 0x%08X ", 4 4
 8B 0C, "      SYS       (%0Ad ms),  E2E Current CRC 0x%08X ", 4 4
 8B 0D, "      SYS       (%0Ad ms),  FW Commit Reset CPU ", 4
 8B 0E, "      SYS       (%0Ad ms),  PS3 Timer=0x%04X ms ", 4 2
 8B 0F, "      SYS       (%0Ad ms),  FW Commit Reset CPU All", 4


;================================================================================
{SetMsgColor = GRAY}
 AA 00, "      debug     (%0Ad ms),  W Commit Interrupt Entry ", 4



