Factory Bad Blocks: 19
-------------------------------------------------------
Sorting FIRMWARE VERVION : S02027
Max Bad Blocks Threshold (per Die) = 100
Max Bad Blocks Threshold (per Plane) = 25
Max Read Fail Blocks Threshold (per Plane) = 25
Max Program Fail Blocks Threshold (per Plane) = 25
Max Erase Fail Threshold (Per Plane) = 25
TLC Read Error Threshold = 80
SLC Read Error Threshold = 30
MaxSfrSucIndex = 0
TSAD = 0x34b
Open Card Temp = 30
-------------------------------------------------------
TOTOAL TIME: 05:28:23
-------------------------------------------------------
====ERROR TYPE====
0 : ECC Fail (Threshold: 80)
1 : ECC FAIL
2 : PROGRAM FAIL
3 : ERASE FAIL
4 : EMPTY PAGE FAIL
5 : NOT EMPTY PAGE FAIL
6 : DATA PATH FAIL
7 : PROGRAM DMA TIMEOUT
8 : READ NAND TIMEOUT
9 : READ DMA DATA TIMEOUT
A : T program
-------------------------------------------------------
====ACTION====
0 : POST READ
1 : PROGRAM
2 : ERASE
3 : EMPTY READ
4 : PARTIAL READ
5 : DISTURB READ
6 : PAGE READ
7 : DATA PATH TEST
8 : 4P PROGRAM
9 : 4P READ
A : 4P ERASE
-------------------------------------------------------
====Error Code====
P05 : BadBlock over spec
P07 : ECC fail Occur
P22 : Program Over Spec
P23 : Erase Over Spec
-------------------------------------------------------
	Bank( L/ P):  1/ 1,  Channel: 2, LUN: 0,  ID: 89 C4 08 32 A6 00 00
	Bad Blocks:0019(0.9%) 
====Total B.B. / Erase Fail / Program Fail / ECC Fail / Factory B.B.====
19 / 0 / 0 / 0 / 19 
====Plane Bad Block Number====
Plane0 BBs = 7
Plane1 BBs = 5
Plane2 BBs = 4
Plane3 BBs = 3
================RDT Bad==================
Bank( L/ P), Channel, LUN, BlockUnit, Plane, Error type, Page,       time, Action, ECC Information,  ErrLoop, ReadLoop , thermal
