MAS1102 MPTool Release Note
///////////////////////////
版本D.0.01.003f改动点说明
MPT：D.0.01.003（SVN863）
GDP: G.00.015(SVN862)
SORT: S.00.015(SVN862)
Utility:U.0.013(SVN0788)
Updater:P.0.07(SVN0702)
Recovery:R.0.03(SVN0744)
Flash:F.08

D.0.01.003f改动点涉及模块说明
MPT：D.0.01.003（SVN863）
1. 增加SMART ID的配置D1/D2/D3/E7(MPTOOL.ini中通过smart enable来使能)

GDP：G.0.015(SVN0862)
1. 修复YMTC9060 CS cache操作的workaround方案

RDT：S.0.015(SVN0862)
1. 修复YMTC9060 CS cache操作的workaround方案

------------------------------------------------------------------------------------------
版本D.0.01.003e改动点说明
MPT：D.0.01.003（SVN842）
GDP: G.00.014(SVN852)
SORT: S.00.014(SVN852)
Utility:U.0.013(SVN0788)
Updater:P.0.07(SVN0702)
Recovery:R.0.03(SVN0744)
Flash:F.08

D.0.01.003e改动点涉及模块说明
GDP：G.0.014(SVN0852)
1. 更新uCode，支持SSV4
2. 更新uCode，支持YMTC9050 mutil-lun

RDT：S.0.014(SVN0852)
1. 修复SSV4 TLC read UNC, 因为dummy page异常
2. 修复RSQ command使用Bank和CE change的issue，支持YMTC9050 mutil-lun

版本D.0.01.003c + D.0.01.003d改动点说明
MPT：D.0.01.003（SVN842）
GDP: G.00.012(SVN839)
SORT: S.00.012(SVN839)
Utility:U.0.013(SVN0788)
Updater:P.0.07(SVN0702)
Recovery:R.0.03(SVN0744)
Flash:F.08

D.0.01.003d改动点涉及模块说明
MPT：D.0.01.003（SVN0842）
1. 支持SSV6或者HynixV6，program code block的次数可配置。（MPTOOL.ini的RDSetting增加SSV6ProgTime=次数）
2. 修改SN input判断SN是否可以允许字母（默认不允许，如果需要在UI中勾选Traget SN栏位下include letter选项）
3. 增加SCY需求，对SCY的bad block做S/C/A的划分（具体需求见jira FAE-2888）
5. 增加对Flash ID的ID6不做判断的配置项（MPTOOL.ini的TestItems增加EnCheckFlashID6=1（默认判断））
6. 修复点击SATA Customize时，SATA parameter无变化的问题

GDP：G.0.012(SVN0839)
1.	增加read parameter page功能
2.	增加nandsweep检查CECH的功能

RDT: S.0.012(SVN0839)
1.	修改FC SDK中polling times的设置值（原来的0xFF改成0xFFF），用于解决某些颗粒出现program fail timeout的问题。

Flash：F.08
1.	更新B47R block num 从2208->2224

版本D.0.01.003 + D.0.01.003b改动点说明
DolphinL MPT D.0.01.003b release at 2021/08/05
1. Utility修改read flash id的功能
2. 增加SATA Parameter可配置功能，默认为2.5、mSATA、M.2各一套，增加手动配置2.5、mSATA、M.2各一套
3. （MPT+RDT）增加SSV6 Code block需要Program twice的配置，可以在MPTool.ini中EnSSV6ProgTwice配置成1生效
4. 修复SN barCode输入确认出现判断异常问题
5. 修复Inherit SN出现多次失败报错弹窗
6. 新增nand sweep失败时，UI显示CECH对应fail的位置，方便客户维修
7. B47R的block数量由原来的2208修改成2224，并支持通过inherit FW/auto Inherit的方式使用2208的FW直接升级到2224的FW
8. 增加read parameter page功能，并在auto detect的UI显示YMTC颗粒的芯片代码
9. 修改自定义SATA PHY参数为点击set，没有保存的问题

DolphinL MPT D.0.01.003b longsys客制化版本修改
1. 修改UI界面上的一些page显示
2. Merge Normal版本的RDT读取方式保证UI不卡顿

版本D.0.01.002d改动点说明
DolphinL MPT D.0.01.002d release at 2021/06/11
1. 增加longsys客制化需求
2. 增加SSV6的支持，SSV6特殊颗粒需要多次prog。通过ini文件中EnSSV6DoubleProg来控制
3. 修复SN barcode的输入确认行为

版本D.0.01.002c改动点说明
DolphinL MPT D.0.01.002c release at 2021/05/07
1. SORT的result增加到1000条数据
2. 读取多张SORT使用线程方式
3. 增加认盘时间的配置
4. 修复Utility显示异常

版本D.0.01.002改动点说明
DolphinL MPT D.0.01.002 release at 2021/03/16
1. 修复Hynix V6识别Flash ID增加set feature切换1.2V
2. 修复A2+YMTC 1.8V在jump to loader会出现卡顿
3. 点击NandSweep Test时增加提示进程图标
4. 修复SORT result 在mutil-lun界面显示不全的问题
5. 增加B47R、YMTC 9060、hynix V6、SSV6的easy retry table，支持这两款nand的easy retry 
6. 修复recovery Tool的download only功能，方便FW调试
7. 增加Updater是否需要内部更新还是外部更新FW version

DolphinL MPT D.0.01.002 RC release at 2021/03/02
1. 修复点击nand sweep test时，软件卡顿问题
2. 支持HynixV6， 增加TMC参数 TMC11用于支持HynixV6
3. 支持SSV6，增加TMC参数 TMC13用于支持SSV6
4. 支持YMTC9060
5. 修复点击auto detect时，由于ucode无法兼容导致软件卡顿的问题
6. 修复Remap使用FW BBB方案时，同一个block出现在三张early bad table、Remap table、BBB table里面
7. 在RDSetting里面增加EnRemapPartialGoodInSLC开关来管理SLC region良率问题，设置0为不启动SLC region功能，不提升良率，设置成1为开启SLC region功能

版本D.0.01.001改动点说明：
DolphinL MPT D.0.01.001 release at 2021/02/25
1. 修改TMC CRC校验不过导致软件多次报错
2. 修复YMTC颗粒，nand sweep不设置0x20无法Low Speed DQS的问题

DolphinL MPT D.0.01.001 RC1 at 2021/02/08
1. 根据会议讨论的一些使用方式做了调整（增加Lock UI功能，无法修改default配置项）
2. 基于DolphinL MPT D.0.00.011a release版本的修改做了整合
3. 修复RDT结果不存在，UI显示异常的问题
4. 保存低速、高速结果到log中

DolphinL MPT D.0.01.001 RC at 2021/02/01
1. 增加低速和高速的calibration方案（一键获取低速、高速结果）
2. TMC由原来“吃文件夹”的方式改成了单一文档管理的方式（仅需要考虑版型）
3. 修改TMC的权限变困难
4. ini不允许被修改，如果新增，请直接复制TMC_ARRAY + 特殊版型号（通过auto detect + force select TMC/Para.ini来手选）
5. Set TMC to array等UI设定，放到Lock UI中。当配置完成Lock UI以后，无法手动修改（具体的使用方式我们组织会议介绍，如果还有不清楚的，请及时告知，我们会再安排一次培训）
6. FW dpd中timing struct修改

===================[20210205]===================
Fix(Test report)
GDP/RDT-0.00.011 (SVN-588) 
    1. Fix jump to fw, sata link error
    
===================[20210201]===================
[NOTE]
	1. If you want to upgrade MPT package from v0.09~v0.09f, v0.10
	   you need to replace (a)MXMPSORT_MAS1102_USB.exe (b)GDP.bin (c)SORT.bin (d)ucode.bin
	   
MPT/SORT/QC/MDI-D.0.00.011(SVN-556)
	1. Modify/Add feature
		a. [NEW FEATURE | MPT] Modify timing struct for Hynix V5/V6 set ddr config. (GDP dependent)
		b. [MINOR ISSUE | MPT] Fix the issue of RW test fail while model name is empty.
		c. [NEW FEATURE | MPT] Add B47R nand type.
		d. [MINOR ISSUE | RDT] Skip 0xAA pattern while get die info to avoid get result hang.
		e. [MAJOR ISSUE | RDT] Modify sorting criteria to include rdt result block. (Per drive - die number, Per die - 1)
		f.[MINOR ISSUE | MPT] Fix RDT pass but MP fail.
		g.[MINOR ISSUE | MPT] Fix scan rdt result fail.
		h.[MINOR ISSUE | MPT] Fix the bug of paritial good remap.

GDP/RDT-0.00.011 (SVN-565)
	1. Modify/Add feature
		a. [NEW FEATURE | GDP] Modify timing struct for Hynix V5/V6 set ddr config.
		b. [NEW FEATURE | GDP] Support A2 chip & SPI function.
		c. [NEW FEATURE | GDP] Support hynix v6 single/mutil-lun.
		d.[NEW FEATURE | GDP] Support B47r.
		e.[NEW FEATURE | RDT] Support hynix v6.
		f.[NEW FEATURE | RDT] Support B47r, but retry funcction is not supported.
		g.[NEW FEATURE | RDT] Support B47r easy retry .
		h. [MINOR ISSUE | RDT] Fix the issue of RDT jump to loader fail.
		i. [MINOR ISSUE | RDT] Fix issue of auto detect fail for B47r.   

Flash.ini-20210107
	1.Add B47R flash information.
	2.Add Hynix v6 single/mutil-lun information.

uCode.bin-20201228
	1. Update Hynix V5/V6 uCode
	2. Add B47R uCode
	3. Add N38A uCode with set feature (debug only)
		
===================[20201221]===================
[NOTE]
	1. If you want to upgrade MPT package from v0.09~v0.09f, 
	   you need to replace (a)MXMPSORT_MAS1102_USB.exe (b)GDP.bin (c)SORT.bin (d)ucode.bin
	   
MPT/SORT/QC/MDI-D.0.00.010(SVN-478)
	1. Modify/Add feature
		a. [MAJOR ISSUE | MPT] Fix RDT DPD loader status, the invalid die with no code block will record as 0xEE.
		b. [MAJOR ISSUE | RDT] Fix RDT result display abnormal issue at jump CE case.
		c. [MAJOR ISSUE | RDT] Modify inherit FW behavior. Erase search do not inherit FW info.				
		d. [NEW FEATURE | MPT] Add a workaround solution to avoid LDR's LDPC UNC page issue.
							   [RDSetting]
							   SKIP_CB=0xF
		e. [NEW FEATURE | MPT] Add a back-door to enable MP with auto-delay. 
							   [RDSetting] 
							   MptFunBitMap=0x4		
		f. [NEW FEATURE | MPT] Add INI to control LDR init driving.
							   [RDSetting]
			                   LDR_PatchDrv0=0x0100002A
							   LDR_PatchDrv1=0x0100002A
		g. [NEW FEATURE | MPT] Add customized features for longsys.				
		h. [NEW FEATURE | MPT] Patch info page to workaround B36R boot fail issue. Enhance controller driving.
		i. [NEW FEATURE | MPT] Add to support get TMC DQSIO Delay from sorting result.
		j. [REFINE      | MPT] Save DPD_D.raw in DPD folder.
		k. [NEW FEATURE | RDT] Add sorting board SPI mode.
		l. [NEW FEATURE | RDT] Add RDT parser get sort result.
		m. [NEW FEATURE | RDT] RDT support ThermalType option.		
		n. [REFINE      | RDT] Remove RDT mode get result CH/CE mapping code 
		o. [MAJOR ISSUE | MPT] By DD/AE's suggestion. Modify nphy_io_rx cs bit as 0
		p. [NEW FEATURE | MPT] add sort bin class for G-tek		
		q. [MINOR ISSUE | MPT] Modify default DQSIO Delay range to 5
		r. [MAJOR ISSUE | MPT] By DD's suggestion to modify TMC formula. 
		s. [MAJOR ISSUE | MPT] By FW's request. Force to mark the last 3 BU to bad for N38A.
		t. [NEW FEATURE | MPT] By FW's request. Add [FwSetting] EnN38ALast3BUBad=0 to control N38A's bad block behavior.
		
GDP/RDT-0.00.010 (SVN-461)
	1. Modify/Add feature
		a. [MAJOR ISSUE | RDT] Fix incorrect bad information display while power-loss after running re-RDT.
		b. [MAJOR ISSUE | RDT] Fixed code block erase issue while CE0, CE1 has no code block.
		c. [MAJOR ISSUE | GDP] Modify set feature flow of nand init for B27B MLUN.		 
		d. [NEW FEATURE | GDP] Support SPI function
		e. [NEW FEATURE | GDP] GDP can read FW programed data. (CFT)
		f. [NEW FEATURE | GDP] GDP can check empty page (CFT)
		g. [NEW FEATURE | GDP] Add new function to skip the specific code blocks of die.		
		h. [NEW FEATURE | GDP] Add loader event case for SPI mode.
		i. [NEW FEATURE | GDP] Support SPI boot fw, mpt flow.
		j. [NEW FEATURE | GDP] Improve MP flow for linux MP. sata_drv_init rx unlock		
		k. [NEW FEATURE | RDT] Support SPI sorting		
		l. [NEW FEATURE | RDT] Improve auto delay flow. We will keep sParam data in RDT result block.
		m. [NEW FEATURE | RDT] Improve sorting function. Interleave program with different pattern per CE 
		n. [NEW FEATURE | RDT] Support internal thermal and add internal/external thermal sensor switch option.
		o. [NEW FEATURE | RDT] RDT Support B36R nand
		p. [MAJOR ISSUE | GDP] Disable un-support sata command to avoid win10 auto detect fail under sata mode.
		q. [NEW FEATURE | RDT] Support GPIO5 to jump loader under sorting board SPI mode. 
		r. [MAJOR ISSUE | GDP] Fix GDP N38A erase fail incomplete issue. 

Utility-0.11
	1. Modify/Add feature
		a. [REFINE      | UTL] By FW's request, modify display string.
		b. [REFINE      | UTL] By customer's request, modify SMART ID info.
		
Updater-0.07
	1. Modify/Add feature
		a. [NEW FEATURE | UPD] Support updater packer tool.
		
Flash.ini-05
	1. Add SSV5 case.
	   
MPTOOL.ini
	1. [ADD] [RDSetting] SKIP_CB=0xF
	2. [ADD] [RDSetting] MptFunBitMap=0x4
	3. [ADD] [RDSetting] LDR_PatchDrv0=0x0100002A LDR_PatchDrv1=0x0100002A

uCode.bin-20201130
	1. [UPDATE] B27B MLUN
	2. [ADD] B47R
	   
===================[20201120]===================
MPT/SORT/QC/MDI-D.0.00.09c(SVN-392)
	1. Modify/Add feature
		a. [MAJOR ISSUE | MPT] Modify REN Delay value by DD's suggestion.

Utility-0.08
	1. Modify/Add feature
		a. [MAJOR ISSUE | UTL] Correct the default and customized information. (SMART INFO)

Flash.ini-04
	1. Add B36R, B27B, YMTC case.

[Effects]
1. Affect FW/GDP/RDT's TMC.
2. Correct Utility display.
3. If you want to upgrade MPT package from v0.09~v0.09b, you can only copy MXMPSORT_MAS1102_USB.exe
		
===================[20201021]===================
MPT/SORT/QC/MDI-A.0.00.09b(SVN-357)
	1. Modify/Add feature
		a. [MAJOR ISSUE | MPT] According to DD's suggestion, modify TMC formula (nphy_io_delay & nifc_dqs_mask)
		
===================[20201020]===================
MPT/SORT/QC/MDI-A.0.00.09a(SVN-355)
	1. Modify/Add feature
		a. [MAJOR ISSUE | MPT] Fix check ID fail issue.
		b. [MAJOR ISSUE | MPT] Fix check GPIO fail issue.
		
===================[20201014]===================
NOTE. MPTOOL.ini is refined and re-ordered at this version.
MPT/SORT/QC/MDI-A.0.00.09(SVN-352)
	1. Modify/Add feature
		a. [REFINE      | MPT] Remove noused MPT.ini
		b. [NEW FEATURE | MPT] Add function to save "nand sweep first" an "KeepTMC" result. [RDSetting] MptFunBitMap=0x2
		c. [NEW FEATURE | MPT] Add feature to check DQSIO delay range for MP use. [TestItems] EnCheckDlyRange=1
		d. [REFINE      | MPT] Modify nand sweep loop from 10 to 30 loop.
		e. [NEW FEATURE | MPT] Add to save dqsio delay value to the record result file.
		f. [REFINE      | MPT] Disable no use UI to avoid the user to feel confuse.
		g. [REFINE      | MPT] fix defect ratio display 
		h. [NEW FEATURE | MPT] add delay for link mode open tool before RDT FW boot
		i. [NEW FEATURE | MPT] add "RDSetting", "MptCusFunBitMap", 0x0  // 0x1: longSys
		j. [REFINE      | MPT] fix sort link mode behavior 
		k. [NEW FEATURE | MPT] add save ecc info data 
		l. [REFINE      | MPT] set Active index Page after start
		m. [REFINE      | MPT] clear code block before erase all
		n. [MAJOR ISSUE | MPT] Fix sort sata connect mode issue 
		o. [MAJOR ISSUE | MPT] Fix BAR_CODE_INPUT_DEVICE_PANEL UI display issue (For M1 BarCodeInputMode requirement)

GDP/RDT-0.00.009 (SVN-351)
	1. Modify/Add feature
		a. [MAJOR ISSUE | GDP] Modify BANK_SHIFT and PAA FAA width to support manual die map. example : 2lun -> 1lun
		b. [MAJOR ISSUE | RDT] Fix multi-lun program fail issue
		c. [MAJOR ISSUE | GDP] Fix Cache read UNC after doing nand sweep first. 
		d. [NEW FEATURE | GDP] Refine nand sweep function.
		e. [NEW FEATURE | GDP] Update ucode define for MPT v0.09.
		f. [MINOR ISSUE | GDP] By Max's suggestion, read status would wait 0xE0.
		g. [REFINE      | GDP] Add FC init function after doing nand sweep first to avoid cache test become slow.
		h. [REFINE      | GDP] Using interleave operation to do cache test to reduce test time.
		i. [MINOR ISSUE | RDT] Fine tune Chip Program function.
		
Utility-0.04
	1. Modify/Add feature
		a. [NEW FEATURE] Add SMART ID 0xF5. (Same as 0xF7)
		b. [NEW FEATURE] Add SMART ID 0xF3.
		
ucode.bin-20200910
	1. Update SSV5 uCode
	2. Update YMTC uCode
	3. Update Hynix V5/V6 uCode

MPTOOL.ini	
	1. [RENAME] [Setting] EnBarCode -> EnSNBarCode
	2. [RENAME] [FwSetting] PageRaid -> EnPageRaid
	3. [RENAME] [FwSetting] Read_Disturb -> ReadDisturb

===================[20200908]===================
[KNOWN ISSUE]
1. [Optional Feature Fail] YMTC nand sweep first fail.
2. [Optional Feature Fail] YMTC RDT sata link mode fail.

MPT/SORT/QC/MDI-A.0.00.08(SVN-317)
	1. Modify/Add feature
		a. [NEW FEATURE | MPT] Update ucode to support SSV5.		
		b. [MINOR ISSUE | MPT] Remove unused menu items.
		c. [NEW FEATURE | MPT] Add FW DPD function1 bit22  DPD_PARAM_FUNCTION_DISABLE_COPY_TASK_CHK
		d. [NEW FEATURE | MPT] Add FW DPD function2 for RD customized feature.
		e. [MAJOR ISSUE | QC ] Fix QC(check temp) MDI(WWN OUI) issue
		f. [NEW FEATURE | MPT] Remove unused files from DAT folder.
		g. [NEW FEATURE | MPT] Rename from DolphinLite to MAS1102.
		h. [NEW FEATURE | MPT] Pass CW size to GDP/RDT from flash.ini spare field.
		i. [NEW FEATURE | MPT] Update YMTC uCode to fix program-without-data command.
		j. [REFINE      | MPT] Fix SCR error address 0xF0328044
		k. [NEW FEATURE | MPT] Sync ANT code base.
		l. [MINOR ISSUE | RDT] Fix erase all check bad number issue.	
		m. [MAJOR ISSUE | RDT] Fix the issue of keep TMC function.
		n. [MAJOR ISSUE | RDT] Fix SORT download issue.
		o. [MAJOR ISSUE | RDT] Fix get Identify_Offset
		
GDP/RDT-0.00.008 (SVN308)
	1.	Modify/Add feature
		a. [MAJOR ISSUE | RDT] Fix YMTC defective bad dectection flow.
		b. [MAJOR ISSUE | RDT] By FW's request, modify randomizer seed for N38A.
		c. [NEW FEATURE | GDP] Add spare byte field to fill into nand_cw_size.
        d. [MAJOR ISSUE | RDT] Refine power throttle setting.
        e. [NEW FEATURE | GDP] Random seed length set from 22 to 64.
		f. [NEW FEATURE | GDP] Add delay for N38A to avoid scan sorting result lost.
		g. [MAJOR ISSUE | RDT] Fix SSV5 RDT nand init fail issue.
		h. [NEW FEATURE | GDP] Support YMTC MLUN.
		i. [MAJOR ISSUE | RDT] Fix the issue of get result block fail on BiCS4.
		j. [NEW FEATURE | RDT] Add HynixV5 TLC shift read command
		k. [NEW FEATURE | GDP] Workaround solution to avoid RW test fail caused by PLD. (FW dependent)
		
Updater-0.05
	1.	Modify/Add feature
		a. [NEW FEATURE] Add scan device button
		b. [MINOR ISSUE] Fix the display of capacity to sync with the behavior of utility.
		c. [NEW FEATURE] Rename from DolphinLite to MAS1102.
		
Utility-0.03
	1.  Modify/Add feature
		a. [NEW FEATURE] Rename from DolphinLite to MAS1102.
		
Flash.ini-03
	1. Renaming BiCS series uniname to match retry table file.
	2. Add spare size field.
	3. Modify N38A GPIO setting.
	4. Add SSV5 32GB die.
	
mem.ini-20200728	
	1. Renaming to sync with flash.ini for BiCS series.

ucode.bin-20200831
	1. Update YMTC uCode.
	2. Update N38A uCode.

Code Block Recovery Tool-A.0.01
	1. Create tool.
	
===================[20200804]===================
MPT/SORT/QC/MDI-A.0.00.07a (SVN280)
	1. Modify/Add feature
		a. [MAJOR ISSUE] According to analog's suggestion. Modify default SATA parameter value. 
		b. [MINOR ISSUE] Apply default value of SATA parameter to UI by SATA connector type.

===================[20200723]===================
MPT/SORT/QC/MDI-A.0.00.07 (SVN275)
	1.	Modify/Add feature
		a. [MAJOR ISSUE / MPT] Fix FW BBB multi-page issue. (This issue is reported at BGL and we had sync it to ANT)
		b. [MAJOR ISSUE / REC] Fix code block recover function.
		c. [MAJOR ISSUE / QC ] Fix QC SN check issue
		d. [NEW FEATURE / MPT] By FW's request, modify remap algorithm for N38A. (The last 3 BU are only for remap)
		e. [NEW FEATURE / MPT] Base on AE's request, modify the nand sweep criteria and refine the UI.
		f. [NEW FEATURE / MPT] Add sort open card Erase All Check Bad
		g. [MINOR ISSUE / MPT] Add Scan USB delay Sec
		h. [MAJOR ISSUE / REC] Fix recovery mode loader block number issue 
		i. [NEW FEATURE / MPT] Enable/disable tool type by ini function bit 
		j. [MAJOR ISSUE / MPT] Inherit sorting result if no code block exists.
		k. [MAJOR ISSUE / MPT] Remove ResPercentage and DefPercentage error message.
		l. [MINOR ISSUE / MPT] Fix barcode input null issue 
		m. [MINOR ISSUE / MPT] Fix auto detect reload TMC ini 
		n. [NEW FEATURE / MPT] By analog's suggestion. Modify default SATA parameter value.
		o. [NEW FEATURE / QC ] Enable test item of check FW DPD.		
		p. [NEW FEATURE / MPT] MPT start check HSPDCapacity value.
		
GDP/RDT-0.00.007 (SVN271)
	1.	Modify/Add feature
		a. [NEW FEATURE] Support WD BiCS4 TLC
		b. [MINOR ISSUE] Delay 1ms(write page) for download only work run
		c. [NEW FEATURE] WD/YMTC nand scan bad block by PageDummyProgram
		d. [NEW FEATURE] Support YMTC X1 and IM B16A nand
		e. [NEW FEATURE] Add YMTC X1 nand support (Add dummy program scan FBB)
		f. [MAJOR ISSUE] Fix nand sweep function for WD BiCS4 TLC.
		g. [MAJOR ISSUE] Modify nand ddr init flow. 
		h. [NEW FEATURE] By analog's suggestion. Modify default SATA parameter value.
		
Flash.ini-02
	1. Modify YMTC scan mode.
