History:
080721 : 08/08/18 release
080722 : 08/08/29 release
	* Turn on sata noise resist register
080826 :
080827 : Support 4BANK with Bank#0/#4/#8/#12 layout configuration. 
  	(Original. support 4-BANK with Bank#0/#1/#4/#5 layout configuration)
081016 :
	1. New support flash: 1)Toshiba G4S; 2)Samsung K9F4G; 3)Hynix H27UBG,H27UCG; 4)Intel 		64GFAMC1,08GAAMC1;
	2. Support SATA HIPM and DIPM slumber/partial mode. (if SlumberEnable=1, default SlumberEnable=0 		in 'JMMassProd.ini')
	3. Add Security Erase (GPIO#1 low active). (if SecurityEraseEnable=1, default 		securityEraseEnable=0 in 'JMMassProd.ini')
	4. Flexible 2~8 channels capacity.
081021 :
	1. Fix S3,S4 security lock.
	2. Add ATA command 0x91 and 0x10 pass Security Lock state
081027 :
	1. Fix power-cycling at wear-leveling