 Shasta+ Release Note, Innogrit Corp.
=====================================
> Date: 2021/02/19

Shasta plus release note (FTK_1.T.V.2Y)
-------------------------------------

01. Reset user ls desc when spb was released due to no data was wrote during rebuilding.

=====================================
> Date: 2021/02/07

Shasta plus release note (FTK_1.T.U.2Y)
-------------------------------------

1. Add ymtc new read retry table by CS2_Read_offset_Rev3.2 doc
2. Add YMTC new read retry table by Read_offset_consumer_Rev3.0 and mask client table temporary
3. Fix Zombie table issue, released open gc spb after rebuild done even if no data was written to this spb
4. Host reading the command took more than 2s to complete
 
=====================================
> Date: 2021/02/03

Shasta plus release note (FTK_1.T.T.2Y)
-------------------------------------

1. Add SanDisk4.5 64GB/die support.

=====================================
> Date: 2021/02/02

Shasta plus release note (FTK_1.T.S.2Y)
-------------------------------------

1. For CDM SeqW Perf, disable some UART log print at SLC appl and release
2. Alloc one more spb for pool1.Increase pool1 gc start thr to 3
3. Revise 512Gb->4T max. pSLC disk size.
4. Fix host read command timeout due to user gc stupid check taking too long on the CPU
5. Pool1 can alloc spb even if free spb count less than block thr value
6. Add report Error for trim CMD waiting in pending queue for more than 6s
 
 
=====================================
> Date: 2021/01/28

Shasta plus release note (FTK_1.T.R.2Y)
-------------------------------------

1. Support sandisk read disturb flow
    (1) support sandisk read disturb flow.
    (2) for sandisk 2T, disable defect remap due to memory issue.
2. Improve user rewrite code.
3. Fix SHARED_DATA memory resource issue for MU 2TB init
    (1) shrink ftl req conut from 32 to 30
4. User gc didnit' start before first convert finish
5. Improve TSB Bics3 512GB SeqW performance to 1500 MBPS
    (1) Disable print log, it will affect SeqW perf

=====================================
> Date: 2021/01/21

Shasta plus release note (FTK_1.T.Q.2Y)
-------------------------------------
01. Fixed backup register(FWSTTS3) are used for sq_count and pmu signature,
           cause remove/install driver create queue fail. Change sq_count -> FWSTTS15
02. Modify pmu mem allocate for CMF fail issue, allocate one section
                 (CMF ENC+DEC) fail will seperate into 2 buffer CMF ENC, CMF DEC.
03. Fixed PMU resume unstable issue.
04. Release back spb which is used at last power cycle. 
 
=====================================
> Date: 2021/01/15

Shasta plus release note (FTK_1.T.P.2Y)
-------------------------------------
01. Disable evlog save feature during fwdownload to prevent msg_isr deadlock

=====================================
> Date: 2021/01/11

Shasta plus release note (FTK_1.T.O.2Y)
-------------------------------------
01. Modify TSB Bics4(32GB/die) nand PHY setting.
 
 
=====================================
> Date: 2021/01/06

Shasta plus release note (FTK_1.T.N.2Y)
-------------------------------------

01. Fixed CMD PROC report CQ full issue.
02. Fixed unhandle read cmd auto lookup result during NVME format.
03. Add vccq_1_2v setting while nand is bics4
04. Change APST table check code.
 
 
=====================================
> Date: 2020/12/30

Shasta plus release note (FTK_1.T.M.2Y)
-------------------------------------

1. Fixed one reboot hang issue during get NAND temperature.
2. Fix bgc deadloop issue
3. Trim command timeout due to flush trim info too late
4. Fix no valid spb issue when test read failed in current write spb
  
=====================================
> Date: 2020/12/25

Shasta plus release note (FTK_1.T.L.2Y)
-------------------------------------

1. Add the fake parameter for sd bics4.5
[Perf] Improve TSB 2T seqW performance to 1050 MBPS.
     (1) Due to write error handle, cache program is disable and it made
         seqW perf drop from 1200 to 450 MBPS.
     (2) allocate ftl_req cnt to 32 for TSB 2TB.
2. Fix timeout issue when write err handling feature disabled
3. Reset middle spb fence to 0 when need flush snapshoot during rebuilding
 
 
=====================================
> Date: 2020/12/18

Shasta plus release note (FTK_1.T.K.2Y)
-------------------------------------

1. Based on HW suggestion, modify TSB/MU/SanDisk PHY setting.
 
=====================================
> Date: 2020/12/16

Shasta plus release note (FTK_1.T.J.2Y)
-------------------------------------

1. Fix PS3/PS4 cannot enter issue
2. Fixed Get feature HMB completion queue entry DW0 should return EHM only.
3. Disable the nand write cache feature for GC to improve data security.
4. Fixed Host HMB segment/size not align to 1M issue.
5. Dataset management command, if trim range start address exceed MaxLBA, then return error status
6. Revise APST check condition for ps_data_entry when ITPT=0 ITPS=0.

 
 
=====================================
> Date: 2020/12/15

Shasta plus release note (FTK_1.T.I.2Y)
-------------------------------------
1. Add sndk bisc4 2T support
2. open odt 100om of soc and drv_str 35om of soc&nand for sandisk bics4.5
 
 
=====================================
> Date: 2020/12/11

Shasta plus release note (FTK_1.T.H.2Y)
-------------------------------------

1. Bypass get Nand PHY DLL lock if NF clock setting to less than 400MHz.
2. Modify NDCU setting for 4byte row address support.
3. Modify ncl_cmd struct to avoid FINST overflow issue for MU 4TB.
4. MU 4LUN package speed is 533MHz.
5. Adjust hmb backup code for reduce TLC write performance drop.
 
=====================================
> Date: 2020/12/09

Shasta plus release note (FTK_1.T.G.2Y)
-------------------------------------

1. Remove error panic
 
 
=====================================
> Date: 2020/12/07

Shasta plus release note (FTK_1.T.E.2Y)
-------------------------------------

1. Fix 5s power loss issue
2. Don't print out "DLL Lock failed" & optimized PLL ready check to 200us.
3. make ls dirty after pad done
4. Don't need to pad if there are no host write and gc write during power cycle

 
 
=====================================
> Date: 2020/12/04

Shasta plus release note (FTK_1.T.D.2Y)
-------------------------------------

1. Adjust memory layout, put part codes to BTCM
2. Reduce pre-assign read performance drop caused by write error handling code
3. Make HDTune Read performance smoothly
   For partial data in, when rtpr reach the end, we backup par_wd[0] to
   pwr_wd[PAR_WD_ENTRY_CNT] for peek at hst_par_wr_done_handler in order to make concatenate smoothly.
 
=====================================
> Date: 2020/12/03

Shasta plus release note (FTK_1.T.C.2Y)
-------------------------------------
1. Fix cirtical gc can't released spb issue
2. Support user data rewrite for nand prog err.
3. Support backup host write data to hmb
4. Internal FW/PCB set P8=1.
5. Fix cirtical gc can't released spb issue
6. Fixed get feature thermal management (tmt1/tmt2) mismatch after set feature.
7. user lut lookup was hang due to lack of dtag
=====================================
> Date: 2020/12/02

Shasta plus release note (FTK_1.T.B.2Y)
-------------------------------------
Alloc buffer to store released flag instead of reuse SPB_DESC_F_DYNAMIC_SLC

=====================================
> Date: 2020/12/01

Shasta plus release note (FTK_1.T.A.2Y)
-------------------------------------

1. Removed SRMA parity warning print.
2. Update ONFi timing mode's t3 to 8. It is more safe, but causes performance drop
 
=====================================
> Date: 2020/11/30

Shasta plus release note (FTK_1.T.9.2Y)
-------------------------------------

1. Fixed VSC CMD vu_ftl_virgin no effect issue.
2. During rebuild, released spb was allced and erased, but spb's desc isn't flush to nand
3. Fixed cpu1 handle ftl_stat_restore(NULL); cause kernel crash issue.
4. Fixed cpu2 not send nvmet_restore_smart_stat() to cpu1 when ftl_virgin issue.
 
=====================================
> Date: 2020/11/27

Shasta plus release note (FTK_1.T.8.2Y)
-------------------------------------

1. Abort/suspend ugc if user flush need pad xlc spb
2. Change mu 2TB timing mode from 10 to 11
3. Add YMTC Vref initial setting for cross temperature during read retry.
4. Modify "ncl_cmd_eh_sim_rec" setting.
5. Add TSB Bics4_272BGA TH58LJ0T24BADE/TH58LJ1T24BAEF support.
6. Improve MU 2TB SeqW performance over 1500 MBPS
    (1) Increase ftl req counts to 32 for MU 2TB
7. Fixed pynvme test ses = 3-7 must return SCT/SC (00/02|01/0A)
 
=====================================
> Date: 2020/11/24

Shasta plus release note (FTK_1.T.7.2Y)
-------------------------------------

1. FW set P5=1 and remove forced GEN3 patch (RC00208A8[4] = 0). For PCIe link stability issue.
2. Fix issue Ra dtag was re-used which casue data miscompare.
 
=====================================
>    Date:              2020/11/23

Shasta plus release note (FTK_1.T.6.2Y)
-------------------------------------
1. Fixed CE remapping handling. Enable CE remap before NDCU mode exit.(ke modification)
2. Store CH/CE remap info. to MR.
3. update loader to support CH/CE remap case.
4. Use SoC temperature-10C as YMTC temperature output.
5. cp dtag can't be released when read back is canceled
6. Keep host write data in order

 
=====================================
>    Date:              2020/11/19

Shasta plus release note (FTK_1.T.5.2Y)
-------------------------------------
1. add read cmd before get temperature fixed read
   nand temperature cause no dqs issue.
2. Sync. pdt_info_misc_t to match RDT/Programmer, add build check.
3. Add mem offset for srb_t and pdt_info_misc_t structure

=====================================
>    Date:              2020/11/17

Shasta plus release note (FTK_1.T.4.2Y)
-------------------------------------
1. Sync the hard reset tPOR with spec for ymtc
2. Fixed YMTC LUN selection for getting temperature.
3. YMTC DQS shall be held high for tDQSRH. Update tCS for YMTC X2.
4. For YMTC use SOC temperature to estimate NAND temperature.
5. Send ltr to host when met command timeout
 
=====================================
>    Date:              2020/11/12

Shasta plus release note (FTK_1.T.3.2Y)
-------------------------------------
1. Fixed SMART temperature sensor1-3 display issue. 1:SOC, 2:NAND, 3:BOARD.
2. Add temperature display select (pdt->specialdebug) default NAND temperature.
3. Fixed hynix nand temperature also return SOC temperature.
 
=====================================
>    Date:              2020/11/11

Shasta plus release note (FTK_1.T.2.2Y)
-------------------------------------
1. cpu2 didn't recieve host write data until first convert complete
2. scan erased page within one WL instead of extra page only
3. Optimized TSB TCL program WCNT.
 
=====================================
>    Date:              2020/11/09

Shasta plus release note (FTK_1.T.1.2Y)
-------------------------------------

1. Bring up hynix 3DV6 NAND.
2. Add the lun select to lun0 in warm reboot.
 
=====================================
>    Date:              2020/11/07

Shasta plus release note (FTK_1.T.0.2Y)
-------------------------------------
1. Fixed read ID issue at DDR3 mode. Both YMTC and Micron NAND had same issue.
2. Force to set 4B ROW address mode for YMTC NAND.
3. Didn't enable thermal interrupt within power on 30s
 
=====================================
>    Date:              2020/11/05

Shasta plus release note (FTK_1.S.0.2Y)
-------------------------------------
1. Set Command abort status queue read ptr equal to write ptr
2. Wait BM idle before force abort running req. Merge from shasta
 
=====================================
>    Date:              2020/11/02

Shasta plus release note (FTK_1.R.0.2Y)
-------------------------------------

1. Added two read ID to workaround YMTC wrong ID issue.
2. Set YMTC 32 DIES's NAND PHY Drive strength to 75ohm.

 
=====================================
>    Date:              2020/10/31

Shasta plus release note (FTK_1.Q.0.2Y)
-------------------------------------

1. Set NFCLK to 200 for TMT2.
2. Cross temp flow improve that set feature from step 0 to step 5 for b16/b27
 
=====================================
>    Date:              2020/10/30

Shasta plus release note (FTK_1.P.0.2Y)
-------------------------------------

1. Fix MU 2T HDTune seqR performance
      - Due to dtag resource, limit dtags to 128 for read ahead for MU 2T
 
=====================================
>    Date:              2020/10/28

Shasta plus release note (FTK_1.O.0.2Y)
-------------------------------------

1. Fixed Get NAND temperature hang issue

=====================================
>    Date:              2020/10/27

Shasta plus release note (FTK_1.N.0.2Y)
-------------------------------------

1. Enhance Fix rlut insert ptr isn't equal with write ptr issue
2. update nf_tcs to 0xF.
 
=====================================
>    Date:              2020/10/26

Shasta plus release note (FTK_1.M.0.2Y)
-------------------------------------

1. Change SNDK BICS4.5 clock to 1066mbps
2. Enhance CDM7 SEQ1M Q1T1 performance to 19xx MBPS
 
=====================================
>    Date:              2020/10/19

Shasta plus release note (FTK_1.L.0.2Y)
-------------------------------------
1. IoMeter 40G perfromance tunning for 256GB MU
 
=====================================
>    Date:              2020/10/16

Shasta plus release note (FTK_1.K.0.2Y)
-------------------------------------
1. Improve IOMeter 40G performance
2. Add pcie compilance/CV test patch
 
=====================================
>    Date:              2020/10/15

Shasta plus release note (FTK_1.J.0.2Y)
-------------------------------------

1. Fix max_req_time overflow issue
 
=====================================
>    Date:              2020/10/14

Shasta plus release note (FTK_1.I.0.2Y)
-------------------------------------

1. Disable cache read for MU B27B 512G disk

=====================================
>    Date:              2020/10/12

Shasta plus release note (FTK_1.H.0.2Y)
-------------------------------------

1. Enable cache read for small capacity disk
2. Enable read refresh for mu nand
3. Fine tune s2s gc parameter of 256GB.
 
=====================================
>    Date:              2020/10/08

Shasta plus release note (FTK_1.G.0.2Y)
-------------------------------------
1. Improve 256GB seq. write speed of MU B27B.
2. Improve PCMark 8 score.
 
=====================================
>    Date:              2020/09/29

Shasta plus release note (FTK_1.F.0.2Y)
-------------------------------------
1. Add vendor SMART function
 
=====================================
>    Date:              2020/09/28

Shasta plus release note (FTK_1.E.0.2Y)
-------------------------------------
1. add ymtc multi-lun support
2. Improve DLL calibration for YMTC NAND.clear
 
=====================================
>    Date:              2020/09/25

Shasta plus release note (FTK_1.D.0.2Y)
-------------------------------------
1. Improve 40G iometer test for seq.


=====================================
>    Date:              2020/09/24

Shasta plus release note (FTK_1.C.0.2Y)
-------------------------------------
1. add ymtc YMN08TB1B1DU1B init code
2. Improve ATA device server password feature set, and add format mek function
 
=====================================
>    Date:              2020/09/22

Shasta plus release note (FTK_1.B.0.2Y)
-------------------------------------
1. 4K write hit the ucache, replace the old data and move the ce to the tail of list

=====================================
>    Date:              2020/09/18

Shasta plus release note (FTK_1.A.0.2Y)
-------------------------------------
1. Fixed memory corruption when srb rebuild.
 
=====================================
>    Date:              2020/09/17

Shasta plus release note (FTK_1.9.0.2Y)
-------------------------------------
1. Fix 256GB can't enter L1.2 due-to SRAM shortage
 
=====================================
>    Date:              2020/09/15

Shasta plus release note (FTK_1.8.0.2Y)
-------------------------------------
1. Don't use 133Mhz to switch NF clock when thermal throttling enters.
2. Fixed NAND TM to 10 for 2T MU NAND. DS to 25ohm.

 =====================================
>    Date:              2020/09/10

Shasta plus release note (FTK_1.7.0.2Y)
-------------------------------------
1. Error remap_idx_len for mu b17 nand


=====================================
>    Date:              2020/09/09

Shasta plus release note (FTK_1.6.0.2Y)
-------------------------------------
1. Moify YMTC test read policy

=====================================
>    Date:              2020/09/08

Shasta plus release note (FTK_1.5.0.2Y)
-------------------------------------
1. fix WL padding can't finish.
2. Enable WL padding

=====================================
>    Date:              2020/09/07

Shasta plus release note (FTK_1.4.0.2Y)
-------------------------------------
1. Don't set NVMe Ready bit when recon is not completed.
 
=====================================
>    Date:              2020/09/05

Shasta plus release note (FTK_1.3.0.2Y)
-------------------------------------
1. Add delay to ensure nand is idle before enable WP
2. Fixed MU B27B NAND timing value.
 
=====================================
>    Date:              2020/08/31

Shasta plus release note (FTK_1.2.0.2Y)
-------------------------------------
1. Set B27 NAND ODT to 50ohm.
2. Updated new Tvalue for 533Mhz.

=====================================
>    Date:              2020/08/20

Shasta plus release note (FTK_1.1.0.2Y)
-------------------------------------
1. Add Opal and ATA device server password feature set.
 
=====================================
>    Date:              2020/08/19

Shasta plus release note (FTK_1.0.0.2Y)
-------------------------------------
1. update MU erd read offset value
2. Fix can't get memory to sleep problem if power domain 1 didn't off.

=====================================
>    Date:              2020/08/16
Shasta plus release note (FTK_1.Q.0.2X)
-------------------------------------
1. Fixed issue: HMB dma timeout during S3/S4 test.

 
=====================================
>    Date:              2020/08/14
Shasta plus release note (FTK_1.P.0.2X)
-------------------------------------
1. Disable TLC erase for SLC block with MU NAND.


=====================================
>    Date:              2020/08/14
Shasta plus release note (FTK_1.O.0.2X)
1. Fixed issue: Host consume too many blocks during test.

 
=====================================
>    Date:              2020/08/13

Shasta plus release note (FTK_1.N.0.2X)
-------------------------------------
1. Enable CPU1 L1 instruction cache when wake-up from L1.2

 
=====================================
>    Date:              2020/08/12
Shasta plus release note (FTK_1.M.0.2X)
-------------------------------------
1. Added padding to multi-plane when backup SPB during reconstruction.
2. Fixed issue: The AER status code returned does not conform to the NVMe spec.

=====================================
>    Date:              2020/08/10
Shasta plus release note (FTK_1.L.0.2X)
-------------------------------------
1. Fixed issue: BSOD when run BurnIn+S3/S4 test.

 
=====================================
>    Date:              2020/08/10
Shasta plus release note (FTK_1.K.0.2X)
-------------------------------------
1. Fixed issue: Correct read page count when scan xlc spb for Micron NAND
2. Fixed issue: Host command timeout when run DM test, normal shutdown need wait write command completion.


=====================================
>    Date:              2020/08/07
Shasta plus release note (FTK_1.J.0.2X)
-------------------------------------
1. Enhance reconstruction handling for SPOR.
  a. Disable cache program during idle flush
  b. Enable erd when reconstruction.
  c. Change idle timer from 2s to 1s

 
=====================================
>    Date:              2020/08/06
Shasta plus release note (FTK_1.I.0.2X)
-------------------------------------
1. Enhance multi-plane aligned write
2. Add timer check do detach HMB if HMB command timeout.

=====================================
>    Date:              2020/08/05
Shasta plus release note (FTK_1.H.0.2X)
-------------------------------------
1. Enable PS3 feature.
2. Enable read resubmit for bm parity error handling.

=====================================
>    Date:              2020/08/04
Shasta plus release note (FTK_1.G.0.2X)
-------------------------------------
1. Improved mininal performance of steady performance test.

 
=====================================
>    Date:              2020/08/03
Shasta plus release note (FTK_1.F.0.2X)
-------------------------------------
1. Fixed issue: read disturb test failure on multipe reads.

 
=====================================
>    Date:              2020/07/31
Shasta plus release note (FTK_1.E.0.2X)
-------------------------------------
1. Fixed issue: Autonomous Power State Transition cannot be disabled

 
=====================================
>    Date:              2020/07/30
Shasta plus release note (FTK_1.D.0.2X)
-------------------------------------
1. Fixed issue: PCIE link down to GEN1 at PCIE expander board.
 
=====================================
>    Date:              2020/07/29
Shasta plus release note (FTK_1.C.0.2X)
-------------------------------------
1. Set flow control to 200MB/s except for 2T Micron.

=====================================
>    Date:              2020/07/28
Shasta plus release note (FTK_1.B.0.2X)
-------------------------------------
1. Added backup over-limit page during reconstruction for SPOR test.

 
=====================================
>    Date:              2020/07/27
Shasta plus release note (FTK_1.A.0.2X)
-------------------------------------
1. Tune SLC to SLC GC performance for Micron NAND.


=====================================
>    Date:              2020/07/25
Shasta plus release note (FTK_1.9.0.2X)
-------------------------------------
1. Support SLC to SLC GC operation.


=====================================
>    Date:              2020/07/24
Shasta plus release note (FTK_1.8.0.2X)
-------------------------------------
1. Fixed issue: trim command timeout.
 
=====================================
>    Date:              2020/07/23
Shasta plus release note (FTK_1.7.0.2X)
-------------------------------------
1. Support ModernStandby feature

 
=====================================
>    Date:              2020/07/22
Shasta plus release note (FTK_1.6.0.2X)
-------------------------------------
1. Enhanced hmb request error handling
 
 
=====================================
>    Date:              2020/07/20
Shasta plus release note (FTK_1.4.0.2X)
-------------------------------------
1. Fixed issue: NCL hang after enter PCIe competion timeout error handle .

 
=====================================
>    Date:              2020/07/17
Shasta plus release note (FTK_1.3.0.2X)
-------------------------------------
1. Fixed issue: partial defect spb write stuck with single die device.
 
 
=====================================
>    Date:              2020/07/16
Shasta plus release note (FTK_1.2.0.2X)
-------------------------------------
1. Fixed issue: IOL test fail due to missed shutdown event during L1.2 entering.
 
 
=====================================
>    Date:              2020/07/13
Shasta plus release note (FTK_1.1.0.2X)
-------------------------------------
1. Improve steady state test performance.

 
=====================================
>    Date:              2020/07/11
Shasta plus release note (FTK_1.0.0.2X)
-------------------------------------
1. Improved HDTune performance

 
=====================================
>    Date:              2020/07/14
Shasta plus release note (FTK_1.A.0.2W)
-------------------------------------
1. Fixed issue: FW reported incorrect temperature.
 
 
=====================================
>    Date:              2020/07/10
Shasta plus release note (FTK_1.9.0.2W)
-------------------------------------
1. Fixed issue: Command timeout when run upgrade + FIO test together on Linux OS.
 
 
=====================================
>    Date:              2020/07/09
Shasta plus release note (FTK_1.8.0.2W)
-------------------------------------
1. Fixed issue: command timeout during FIO test.
 
 
=====================================
>    Date:              2020/07/03
 
Shasta plus release note (FTK_1.6.0.2W)
-------------------------------------
1. Fixed issue: Can't enter L1.2 on 2TB drive.

 
=====================================
>    Date:              2020/07/02
Shasta plus release note (FTK_1.5.0.2W)
-------------------------------------
[FW UPDATE]
1. Fixed issue: FW set incorrect subvid and did.
 
 
=====================================
>    Date:              2020/06/30
Shasta plus release note (FTK_1.4.0.2W)
-------------------------------------
1. Fixed issue: FW hit panic when no enough memory.
 
 
=====================================
>    Date:              2020/06/29

Shasta plus release note (FTK_1.3.0.2W)
-------------------------------------
1. Enhanced read disturb policy to avoid read error issue.

 
 
=====================================
>    Date:              2020/06/28
Shasta plus release note (FTK_1.2.0.2W)
-------------------------------------
1. Support YMTC 64L TLC NAND.
 
 
=====================================
>    Date:              2020/06/25
Shasta plus release note (FTK_1.1.0.2W)
-------------------------------------
1. Fixed issue: Dual CPU message hang during stress test.

 
=====================================
>    Date:              2020/06/24
Shasta plus release note (FTK_1.0.0.2W)
-------------------------------------
1. Fixed SPOR issue, keep write in oder and rollback command paritial data.
  
=====================================
>    Date:              2020/06/01

Shasta plus release note (FTK_1.1.0.2V)
-------------------------------------
1. Enable HMB auto-lookup table to improve performance.
 
 
=====================================
>    Date:              2020/05/31

Shasta plus release note (FTK_1.0.0.2V)
-------------------------------------
1. Adjust Core/PHY LDO setting for FTK.

=====================================
>    Date:              2020/05/30

Shasta plus release note (FTK_1.0.0.2U)
-------------------------------------
1. Fixed issue: Host was stopped sometimes when run S3/S4 test.
2. Fixed download issue on 2TB SSD.
3. Enable read disturb handling.
4. Optimize PCIe reset handling flow and avoid long time detection sometimes.
5. Support Micron B27B 4 LUN NAND.
6. Fixed issue: erase error status was not clear on Micron NAND.
7. Fixed issue: DM NT3 FW download test failure.
8. Fixed issue: NAND data was wrong sometimes on one TSB NAND. NAND timing setting issue.
 
=====================================
>    Date:              2020/05/09

Shasta plus release note (FTK_1.0.0.2T)
-------------------------------------
1. Support set/get VID/DID via MP tool.
 
 
=====================================
>    Date:              2020/05/08
Shasta plus release note (FTK_1.0.0.2S)
-------------------------------------
1. Initial version for DVT test.
﻿