2010.06.10
1、update MP_Tool，fix d bug for AutoRun.
2010.05.31
1.修改3D1D CLOCK 00 00
2010.05.28
1.修正0526的问题
2010.05.26
1.更新page mode的ISP 解决超稳定问题；
2.更新sec  mode 的ISP 解决4D2E format fail问题
3.解决3D2E flash pret fail问题，FORCE 5T2F flash option 0x26
2010.05.21
1.5D2F flash option26
2.修改容量优先
3.hynix 128MB option20

2010.05.13
force 3d2e flash   toshibaaddr,toshiba command option 23
2010.05.07
1.更新data base 删除多余的
2.修改tool exe 解决开卡clock传错误问题
2010.05.05
1.support 6D2F flash modify only data base
2.modify 98 D5 94 BA CLOCK 90 90
2010.05.04
此版本是容量优先的sorting
1.support sansung C die flash
2.support TC58NVGOS3ETA00 flash

2010.04.30
1、update database(98 D3 84 32);
2010.04.16
1.修改toshiba data base osc clock
2.更新MPTool；
3.修正多CE Pretest code和ISP code；
4.Toshiba 1plane强制为samsung address mode。
2010.04.15
1.解决 2CE L63A FLASH 问题以及修正time out 的处理
2.toshiba one plane option 设置为 0x26
2010.04.13
解决 2CE L63A FLASH 低格开卡问题  修改CE ON AND OFF配对数目
2010.04.13
解决 2CE L63A FLASH 开卡问题
SUPPORT ID 0x45,0xF1,0x84,0x95  FLASH
2010.03.25
修改3211BC1 3FF block 不用
2010.03.22
解决HYNIX 256MB SLC 开卡 FAIL
跟新downgrad MPTOOL 对ERASR ALL BLOCK AND ERASE GOOD BLOCK SLECT
2010.03.09
解决SEC 0 坏的固定容量问题，修改工具
2010.03.04
1.support L74 flash
2.support ID 0x98,0xDE,0x95,0x32 flash
3.fix a bug of 所有的SEC 是坏的 一个BUG
4.修改SEC的ISP code 处理多PORT 的问题 
2010.02.03
1.支持BC2分位， 但是SEC MODE 的flash 在BC1硬件上DOWN ISP 会有问题
2010.02.03
1.修正CE0是坏的BUG
2.支持SEC0 BAD
2010.02.02
1.flash id 2c d7 94 3e flash ce0 坏的支持
2009.01.29
1、Fix a bug in pretest.(pretest code)
2010.01.27
1、update data base to support Micron(2C D3 90 2E) flash.(Data base)
2、fix a bug for page 256 in sector mode.(ISP)
2010.01.25
1.update sorting 里的PAGE MODE 的选择
2010.01.22
1、add two new parameters(sector Bad bound and improve bad block count per mu)(mptool and pretest code)
2010.01.20
1、support TC58NVG5D2FTAIO flash
2、support H27UBG8T2A flash
3、MODIFY Auto_Ale.H page256 set address
4、update sector mode flash isp bin
2010.01.20
1、fix a bug for toshiba flash default cardmode addr(preautof.c);
2、fix a bug for ispwrite function;
2010.01.15
1、fix a bug for ChipGenius Tool can't recognize the PID &Serial Number;
2、update MP_Tool for MUti Language. 
2010.01.14
1.fix the bug of micron 4ce flash force strong page is special2
2.延长RB的等待时间;
3.ignore read fail while serial num is zero and fill up new pages with zero
2010.01.07
1、modify o_pret sorting method(MU-BLK-P);
2010.01.07
1、延长RB的等待时间;
2、Do not always use copy back for 8K flash(see 2009.12.28 )；
3、modify setor mode performance;
4、add to support M61 Flash(2C 28 00 26);
2010.01.04
1、fix the HDD issue
2009.12.31
1、fix a bug of build link table;
2、fix the RB Timeout issue;
3、improve the sorting method(do not care the fail mu).
2009.12.29
1、update the MP_Tool.
2009.12.28
1、Set Copy Back flag for Page 8K flash.(pretest and ISP)
2009.12.25
1、Fix a bug in mark bad isp.(ISP)
2009.12.18
1、Add new ID.(database and pretest)
2、fix a bug in Format.(pretest)
2009.12.16
1、Fix a bug which cause h2test fail without marking bad blocks.(ISP)
2009.12.09
1、Fix a bug for 2plane.(pretest)
2009.12.07
1、Fix a bug for page 8K.(pretest)
2、Update card mode for toshiba 6D2E flash.(pretest)
2009.12.07
1、add Read Only function (fix a isp bug);
2、make uinit.bin save in strong page;
2009.12.04
1、fix a isp code bug(无法写入厂商信息)
2009.12.01
1、open open_short_test for original.(mptool_I1201_V2.02.05v3)
2、Fix a bug in download parameters.(mptool_I1201_V2.02.05v4)
2009.11.30
1、Fix a bug in showing mode.(mptool_I1130_V2.02.05v3)
2、Fix a bug in showing color.(mptool_I1130_V2.02.05v3)
3、add two new input parameters for downgrade.(pretest and mptool_I1130_V2.02.05v3)
4、open open_short_test for downgrade,close open_short_test for original.(mptool_I1130_V2.02.05v3)
2009.11.26
1、Add a new parameter,Erase_All_Block,for original、Lev11 and Lev12(pretest code)
2、Fix a bug in open short test.(open short test code)
3、close open short function.(MPTool I1126 V1)
4、Fix a bug whick cause errors in detecting L63A Flash ID.(MPTool I1126 V1)
2009.11.25
1、close power cycle function in downgrade(ISP code)
2009.11.24
1、add open short test.(mptool I1124_V1)
2、download parameters no matter downgrade or original.(mptool I1124_V2)
3、open power cycle function.(ISP code)
4、fix a bug for open short test.(mptool I1124_V2)
5、select downgrade mode in "Setting",if you want to use open short test function.
2009.11.23
1、add open_short function in "Others Setting".(mptool and code)
2、update database to support new flash.(MT29F128G08TAA and some sandisk flashes)(mptool and pretest)
3、download a short ISP code to get the address of ISP block.(mptool and code)
2009.11.20
1、add the whole mode ;
2009.11.09
1、add "erase all block" input parameter in "Setting".(mptool)
2009.09.28
1、add lev09
2009.09.23
1、update MP_Tool can auto scan BC and BC1
2009.0909
1、Update ISP and Pretest to support Hynix 41nm Flash with single plane.
2、Don't support 8K 2plane.
2009.09.03
1、update to support orginal flash.
2009.08.27
1、Fix a bug in ISP write、clean mother and clean fat for 8K 1 plane.
2009.08.26
1、Update ISP code for 8K flash with page mode. Not support 8K 2plane.
2、Update mp tool.
2009.08.18
1、update MP_Tool ,ignore badblockoversetting;
2、update DBF file.
2009.08.11
1、fix a bug of pretest SectorA=0.
2. Supported Original flash(support 2plane and intinlve).
2009.08.04
1、Modify definition of RandomSeed addr in a more friendly way
2、Only write 55-aa for spare area of sector 0
2009.07.31
1、Change pattern of random generator.
2、write 55-aa for any sector while writing pattern
3、remove support of any page mode
2009.07.30
1、Change clk of l62,l63,T43nm to 90 in dbf file.
2、Make pattern the same with SD.
2009.07.21
1、fix a bug of set the wrong ignore status of ISP.
2、enhance sorting for any mode.
3、get ecc mode from mptool
2009.07.20
1、Let all scan modes OK. 
2、Fix a bug of preformating.
3、Fix some bugs of ISP.
2009.07.13
1、add 8k and 256 page support. 8k is only supported with scan mode 2 now. 
2009.07.03
1、add 256 page support for original flash (only ISP)
2009.06.30
1、fix a bug of 3211 original pretest
2009.06.25
1、add 3211 pretest and isp bin
2009.06.18
1、update SM3252bb Level07.
2009.06.12
1、update SM3251AB/BA Level07(this version is the same as I0316's version,but will chk spr0==0 or    other),Level08,Level10,Level11,Level15;(will chk spr0==0 or other)
2、update SM3252BB Level07;(will chk spr0==0 or other)
3、update SM3252BB isp code about static capacity;
2009.5.21//Tiger
1、add level07 for 3252C.(same with level07, but only run 1 plane mode)
2009.5.20//Tiger
1、add level06 for 3252C.(normal scan + multi times weakpage scan. If full capacity,run 1 plane.If half capacity,run 2 plane)
2009.05.25
1、Close Inteleve Mode (isp&pretest) for Toshiba 43nm:update level09,level99 and isp code;
2009.05.12
1、update MP_Tool :when select Level99 will match Toshiba 43nm isp code.
2009.05.11
1、add level99 for Toshiba 43nm flash;
2009.04.27
1、fix a bug of DG code when half capacity flash  in windows2000 system can't format(close wear-leveling code in    uinit() function),update DG isp code;
2009.04.22
1、add level08(like Alcor)
2009.04.20
1、fix level07,if erase fail will mark bad;
2、fix FLASHID=2C D7 94 3E flash,w/r clk to 90;
2009.04.01
1 fix Level89,add more weak page
2009.03.20
1、fixed level07&level89 for Intel 34nm:if bad block numbers is more than 352(1plane) or 176(2plane) in first W/R,it will check ecc bit in the following operation.
2009.03.17
1、MP_tool adds the function about Level81~Level90 load 2 plane isp code.
2、change I0316 version's Level90 to Level89(pretest and isp are both run 2plane);
3、change I0316 version's Level8 to Level88(pretest runs single plane,and isp runs 2plane);
4、add level90(this level is just load the info block's bad info,and run 2plane);
5、ignore erase and program fail in isp code;
6、fixed Level1~Level100(except level09),when save info block,saved level and eccbit info;
2009.03.16
1、add SM3252B folder for Toshiba 43nm ForceID
2009.03.15
1、for level90,will read status when write one page;
2、change level07(just like level11 but will rewrite some weakpage),run single plane;
3、add level08,run single plane to do pretest,and ISP code runs 2plane;
2009.03.14
1、write weak page again for Level90;
2、run single plane to erase for Level90;
3、add level07 for Intel34nm ,run single plane.
2009.03.11
1、fixed a bug of level03(SM325A/B);
2、add level06(pattern is 0x55,0xaa);
2009.03.10
1、Change the R/W clk from 00 to 90 for  Intel 34nm DG Flash ;
2、Change Level90 to support Intel 34nm DG Flash(it will run 2 plane mode to scan the flash);
2009.03.06
1、For SM3252A DG Flash ,change Level12 to Level15;
2009.03.05
1、Modify Level80 pretest code,it writes 3 times and the last just for the odd page;
2009.03.03
1、add SM325AC Level80 to support AGAND DownGrade FLASH;
2、Modify SM325AC DownGrade isp code;
2009.03.02
1、add orginal bin file to support AGAND FLASH;
2009.02.13
1、Modify the clk from 00 to 80 for Mrcion 34nm;
2、Add level05 for Mrcion 34nm;
2009.02.09
1、 extend the pretest time out to 60 mins.
2009.02.08
1、Modify level90 run 2plane just mark the orginal bad block;
2、Modify level100 run single plane just mark the orginal bad block;
2009.01.16
1、Modify level02&level03 ,all the program action is running two plane mode to improve the speed;
2、Modify level09 for Toshiba 43nm ,the reserve block change to 10;
2009.01.14
1、level02 is from level01 for Mrcion;
2、level03 is from level01 for Intel;
2009.01.07
1、fix a bug of pretest code;
2008.12.31
1、add Mrion 34nm
2008.12.25
1、Toshiba 43nm:open ignore erase&program and change pattern;
2、update Toshiba 43nm isp code;
 ps:
   level04: for G-Tek DG Flash will be better(is level12 change pattern);
   level09: is just for Toshiba 43nm.
2008.12.16
1. support toshiba 43nm DG flash in Level 9;
2. add  level 01 for more stick test pattern for Hopestar.

Ps: Level 10:  Write 2plane; read 1plane
    Llevel 11:  write/read 1plane
    Level 12:  page compare + block compare.
    Level 100: refer the original bad, 1 plane
    Level 90: refer the original bad , 2plane


2008.06.25
  1.Modify Clock Setting in DBF file
    *divide 0x180 bit5 write clock by 2
    *divide 0x181 bit6 read clock by 2
    *divide 0x180 bit6 read clock by 2
冘2.Modify Pattern Level 7, which is faster flash initialization than Level 11


2008.06.10
  1. Improve scan performance
  2. Improve yield rate
  3. Update flash test pattern LV8, LV9, and LV10
  4. Default set to LV10

2008.05.15
  1. Add Level 100

2009.05.09

  1. Improve Stability
  2. Update DBF table

2008.02.27
  Here are the update and release note:
  1. Update ISP to align with latest ISP(G1228)
  2. Improve Fast Flash Initialization
  3. Modify LED display 
  4. Update Flash test pattern Level 11, 12, 13

