[ForceFW]
FLASH_ALL_PTIF=0

//--- Intel L06
FLASH_89A46432AA01_ISP=SM3281BB_ISP_MLC_L06.BIN
FLASH_89A46432AA01_PTEST=PT.bin
FLASH_89A46432AA01_BootCode=BootCode.bin
FLASH_89A46432AA01_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_L06.bin

//--- Micron L85/L95
FLASH_2C846454A900_ISP=SM3281BB_ISP_MLC_L85c.BIN
FLASH_2C846454A900_PTEST=PT.bin
FLASH_2C846454A900_BootCode=BootCode.bin
FLASH_2C846454A900_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_L06.bin

//---
FLASH_2C84643CA904_ISP=SM3281BB_ISP_MLC_L85c.BIN
FLASH_2C84643CA904_PTEST=PT.bin
FLASH_2C84643CA904_BootCode=BootCode.bin
FLASH_2C84643CA904_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_L06.bin
//--- Micron L06
FLASH_2CA46432AA04_ISP=SM3281BB_ISP_MLC_L06.BIN
FLASH_2CA46432AA04_PTEST=PT.bin
FLASH_2CA46432AA04_BootCode=BootCode.bin
FLASH_2CA46432AA04_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_L06.bin

//--- Micron L05
FLASH_2C844434AA00_ISP=SM3281BB_ISP_MLC_L06.BIN
FLASH_2C844434AA00_PTEST=PT.bin
FLASH_2C844434AA00_BootCode=BootCode.bin
FLASH_2C844434AA00_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_L06.bin

//--- Micron B05
FLASH_2C84D832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2C84D832A100_PTEST=PT.bin
FLASH_2C84D832A100_BootCode=BootCode.bin
FLASH_2C84D832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B05
FLASH_2C845832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2C845832A100_PTEST=PT.bin
FLASH_2C845832A100_BootCode=BootCode.bin
FLASH_2C845832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B16
FLASH_2CA40832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CA40832A100_PTEST=PT.bin
FLASH_2CA40832A100_BootCode=BootCode.bin
FLASH_2CA40832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B16
FLASH_2CA48832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CA48832A100_PTEST=PT.bin
FLASH_2CA48832A100_BootCode=BootCode.bin
FLASH_2CA48832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B16
FLASH_2CC48932A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CC48932A100_PTEST=PT.bin
FLASH_2CC48932A100_BootCode=BootCode.bin
FLASH_2CC48932A100_RETRYBIN=PS_SRTY\PS_SRTY_L06.bin

//--- Micron B17
FLASH_2CD48932A600_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CD48932A600_PTEST=PT.bin
FLASH_2CD48932A600_BootCode=BootCode.bin
FLASH_2CD48932A600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B17
FLASH_2CC40832A600_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CC40832A600_PTEST=PT.bin
FLASH_2CC40832A600_BootCode=BootCode.bin
FLASH_2CC40832A600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B17
FLASH_2CC40832A601_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CC40832A601_PTEST=PT.bin
FLASH_2CC40832A601_BootCode=BootCode.bin
FLASH_2CC40832A601_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B27A
FLASH_2CC40832A200_ISP=SM3281BB_ISP_TLC_B27A.BIN
FLASH_2CC40832A200_PTEST=PT.bin
FLASH_2CC40832A200_BootCode=BootCode.bin
FLASH_2CC40832A200_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_B27A.bin

//--- Micron B27A
FLASH_2CC41832A200_ISP=SM3281BB_ISP_TLC_B27A.BIN
FLASH_2CC41832A200_PTEST=PT.bin
FLASH_2CC41832A200_BootCode=BootCode.bin
FLASH_2CC41832A200_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_B27A.bin

//--- Micron B27B
FLASH_2CC30832E600_ISP=SM3281BB_ISP_TLC_B27A.BIN
FLASH_2CC30832E600_PTEST=PT.bin
FLASH_2CC30832E600_BootCode=BootCode.bin
FLASH_2CC30832E600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_B27A.bin

//--- Intel B16
FLASH_89A40832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_89A40832A100_PTEST=PT.bin
FLASH_89A40832A100_BootCode=BootCode.bin
FLASH_89A40832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B17
FLASH_89C40832A600_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_89C40832A600_PTEST=PT.bin
FLASH_89C40832A600_BootCode=BootCode.bin
FLASH_89C40832A600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B17
FLASH_2CD48932A601_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CD48932A601_PTEST=PT.bin
FLASH_2CD48932A601_BootCode=BootCode.bin
FLASH_2CD48932A601_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B17
FLASH_2CE48A32A600_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CE48A32A600_PTEST=PT.bin
FLASH_2CE48A32A600_BootCode=BootCode.bin
FLASH_2CE48A32A600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Intel N18
FLASH_89D40C32AA00_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_89D40C32AA00_PTEST=PT.bin
FLASH_89D40C32AA00_BootCode=BootCode.bin
FLASH_89D40C32AA00_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron N18
FLASH_2CD40C32AA00_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CD40C32AA00_PTEST=PT.bin
FLASH_2CD40C32AA00_BootCode=BootCode.bin
FLASH_2CD40C32AA00_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron N28A
FLASH_2CD31C32C600_ISP=SM3281BB_ISP_QLC_N28.BIN
FLASH_2CD31C32C600_PTEST=PT.bin
FLASH_2CD31C32C600_BootCode=BootCode.bin
FLASH_2CD31C32C600_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Micron B37R
FLASH_2CC37832EA10_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_2CC37832EA10_PTEST=PT.bin
FLASH_2CC37832EA10_BootCode=BootCode.bin
FLASH_2CC37832EA10_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Speteck B16
FLASH_B5A40832A100_ISP=SM3281BB_ISP_TLC_B16.BIN
FLASH_B5A40832A100_PTEST=PT.bin
FLASH_B5A40832A100_BootCode=BootCode.bin
FLASH_B5A40832A100_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_L06.bin

//--- Samsung 3D V4
FLASH_EC1C983F84CB_ISP=SM3281BB_ISP_TLC_SS_3D_V4_AFG.BIN
FLASH_EC1C983F84CB_PTEST=PT.bin
FLASH_EC1C983F84CB_BootCode=BootCode.bin
FLASH_2CE48A32A600_RETRYBIN=PS_SRTY\PS_CopyBack_SS_3D_SRTY_SS_TLC_3D_AFG.bin

FLASH_EC1E983F84CB_ISP=SM3281BB_ISP_TLC_SS_3D_V4_AHG.BIN
FLASH_EC1E983F84CB_PTEST=PT.bin
FLASH_EC1E983F84CB_BootCode=BootCode.bin
FLASH_2CE48A32A600_RETRYBIN=PS_SRTY\PS_CopyBack_SS_3D_SRTY_SS_TLC_3D_AHG.bin

//--- Samsung 14 MLC
FLASH_EC3A94C3A4CA_ISP=SM3281BB_ISP_MLC_SS_14nm.BIN
FLASH_EC3A94C3A4CA_PTEST=PT.bin
FLASH_EC3A94C3A4CA_BootCode=BootCode.bin
FLASH_EC3A94C3A4CA_RETRYBIN=PS_SRTY\PS_CopyBack_SS_3D_SRTY_SS_TLC_3D_AFG.bin

//--- HY 14nm MLC
FLASH_AD3A14030850_ISP=SM3281BB_ISP_MLC_HY_14nm.BIN
FLASH_AD3A14030850_PTEST=PT.bin
FLASH_AD3A14030850_DisableCardModeFW=1
FLASH_AD3A14030850_BootCode=BootCode_HY.bin


//--- HY 3D V3 (8M3M)
FLASH_AD5C28BA0080_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5C28BA0080_PTEST=PT.bin
FLASH_AD5C28BA0080_DisableCardModeFW=1
FLASH_AD5C28BA0080_BootCode=BootCode_HY.bin

//--- HY 3D V3 (8M3M)
FLASH_AD5C28BA0080_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5C28BA0080_PTEST=PT.bin
FLASH_AD5C28BA0080_DisableCardModeFW=1
FLASH_AD5C28BA0080_BootCode=BootCode_HY.bin

//--- HY 3D V4 (8M2A)
FLASH_AD5C282A0190_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5C282A0190_PTEST=PT.bin
FLASH_AD5C282A0190_DisableCardModeFW=1
FLASH_AD5C282A0190_BootCode=BootCode_HY.bin

//--- HY 3D V4 (8A1A)
FLASH_AD5E28221090_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5E28221090_PTEST=PT.bin
FLASH_AD5E28221090_DisableCardModeFW=1
FLASH_AD5E28221090_BootCode=BootCode_HY.bin

//--- HY 3D V5 (8A1M)
FLASH_AD5E283300A0_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5E283300A0_PTEST=PT.bin
FLASH_AD5E283300A0_DisableCardModeFW=1
FLASH_AD5E283300A0_BootCode=BootCode_HY.bin

//--- HY 3D V6 (H25JGT8A1M8R)
FLASH_AD89285300B0_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD89285300B0_PTEST=PT.bin
FLASH_AD89285300B0_DisableCardModeFW=1
FLASH_AD89285300B0_BootCode=BootCode_HY.bin

//--- HY 3D V6 (H25BFT8A1B8R)
FLASH_AD5E285302B0_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD5E285302B0_PTEST=PT.bin
FLASH_AD5E285302B0_DisableCardModeFW=1
FLASH_AD5E285302B0_BootCode=BootCode_HY.bin

//--- HY 3D V6 (H25BFT8A1B8R)
FLASH_AD7E285302B0_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD7E285302B0_PTEST=PT.bin
FLASH_AD7E285302B0_DisableCardModeFW=1
FLASH_AD7E285302B0_BootCode=BootCode_HY.bin

//--- HY 3D V5 QLC (H25JGQ8A1M8R)
FLASH_AD892C5330A0_ISP=SM3281BB_ISP_TLC_HY.BIN
FLASH_AD892C5330A0_PTEST=PT.bin
FLASH_AD892C5330A0_DisableCardModeFW=1
FLASH_AD892C5330A0_BootCode=BootCode_HY.bin

//--- Sandisk 3D Bics3
FLASH_453A98B37672_ISP=SM3281BB_ISP_TLC_SD_3D_Bics3_128Gb.BIN
FLASH_453A98B37672_PTEST=PT.bin
FLASH_453A98B37672_BootCode=BootCode.bin
FLASH_453A98B37672_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics3_128Gb.bin

FLASH_453C98B37672_ISP=SM3281BB_ISP_TLC_SD_3D_Bics3_256Gb.BIN
FLASH_453C98B37672_PTEST=PT.bin
FLASH_453C98B37672_BootCode=BootCode.bin
FLASH_453C98B37672_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics3_256Gb.bin

FLASH_453E98B37672_ISP=SM3281BB_ISP_TLC_SD_3D_Bics3_512Gb.BIN
FLASH_453E98B37672_PTEST=PT.bin
FLASH_453E98B37672_BootCode=BootCode.bin
FLASH_453E98B37672_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics3_512Gb.bin

FLASH_453E99B37A72_ISP=SM3281BB_ISP_TLC_SD_3D_Bics3_256Gb.BIN
FLASH_453E99B37A72_PTEST=PT.bin
FLASH_453E99B37A72_BootCode=BootCode.bin
FLASH_453E99B37A72_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics3_256Gb.bin

FLASH_45489AB37E72_ISP=SM3281BB_ISP_TLC_SD_3D_Bics3_256Gb.BIN
FLASH_45489AB37E72_PTEST=PT.bin
FLASH_45489AB37E72_BootCode=BootCode.bin
FLASH_45489AB37E72_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics3_256Gb.bin

//--- Sandisk 3D Bics4

FLASH_453C98B37663_ISP=SM3281BB_ISP_TLC_SD_3D_Bics4_256Gb.BIN
FLASH_453C98B37663_PTEST=PT.bin
FLASH_453C98B37663_BootCode=BootCode.bin
FLASH_453C98B37663_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics4_256Gb.bin

FLASH_453C98B3766B_ISP=SM3281BB_ISP_TLC_SD_3D_Bics4_256Gb.BIN
FLASH_453C98B3766B_PTEST=PT.bin
FLASH_453C98B3766B_BootCode=BootCode.bin
FLASH_453C98B3766B_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics4_256Gb.bin

FLASH_453E98B37663_ISP=SM3281BB_ISP_TLC_SD_3D_Bics4_512Gb.BIN
FLASH_453E98B37663_PTEST=PT.bin
FLASH_453E98B37663_BootCode=BootCode.bin
FLASH_453E98B37663_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics4_512Gb.bin

FLASH_453E98B3766B_ISP=SM3281BB_ISP_TLC_SD_3D_Bics4_512Gb.BIN
FLASH_453E98B3766B_PTEST=PT.bin
FLASH_453E98B3766B_BootCode=BootCode.bin
FLASH_453E98B3766B_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_SD_TLC_3D_Bics4_512Gb.bin

//--- SanDisk 15nm MLC
FLASH_453A94937651_ISP=SM3281BB_ISP_MLC_SD_15nm.BIN 
FLASH_453A94937651_PTEST=PT.bin
FLASH_453A94937651_BootCode=BootCode.bin
FLASH_453A94937651_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_SD_MLC_15nm.bin

FLASH_453AA4937A51_ISP=SM3281BB_ISP_MLC_SD_15nm.BIN
FLASH_453AA4937A51_PTEST=PT.bin
FLASH_453AA4937A51_BootCode=BootCode.bin
FLASH_453AA4937A51_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_SD_MLC_15nm.bin

//--- SanDisk 15nm MLC
FLASH_453C95937A51_ISP=SM3281BB_ISP_MLC_SD_15nm.BIN
FLASH_453C95937A51_PTEST=PT.bin
FLASH_453C95937A51_BootCode=BootCode.bin

FLASH_453CA5937E51_ISP=SM3281BB_ISP_MLC_SD_15nm.BIN
FLASH_453CA5937E51_PTEST=PT.bin
FLASH_453CA5937E51_BootCode=BootCode.bin
FLASH_453CA5937E51_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_SD_MLC_15nm.bin

FLASH_453EA6937E51_ISP=SM3281BB_ISP_MLC_SD_15nm.BIN
FLASH_453EA6937E51_PTEST=PT.bin
FLASH_453EA6937E51_BootCode=BootCode.bin
FLASH_453EA6937E51_RETRYBIN=PS_SRTY\PS_CopyBack_MLC_SRTY_SD_MLC_15nm.bin

//--- SanDisk 15nm TLC
FLASH_454C98A37651_ISP=SM3281BB_ISP_TLC_SD_15nm.BIN 
FLASH_454C98A37651_PTEST=PT.bin
FLASH_454C98A37651_BootCode=BootCode.bin
FLASH_454C98A37651_RETRYBIN=PS_SRTY\


//--- Toshiba 3D Bics4
FLASH_983C98B376E3_ISP=SM3281BB_ISP_TLC_T_3D_Bics4_256Gb.BIN
FLASH_983C98B376E3_PTEST=PT.bin
FLASH_983C98B376E3_BootCode=BootCode.bin
FLASH_983C98B376E3_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_T_TLC_3D_Bics4_256Gb.bin

//--- Toshiba 3D Bics4 512Gb
FLASH_983E98B37663_ISP=SM3281BB_ISP_TLC_T_3D_Bics4_512Gb.BIN
FLASH_983E98B37663_PTEST=PT.bin
FLASH_983E98B37663_BootCode=BootCode.bin
FLASH_983E98B37663_RETRYBIN=PS_SRTY\PS_CopyBack_IM_SRTY_T_TLC_3D_Bics4_512Gb.bin

//--- YMTC TLC
FLASH_9BC348251000_ISP=SM3281BB_ISP_TLC_YMTC.BIN
FLASH_9BC348251000_PTEST=PT.bin
FLASH_9BC348251000_BootCode=BootCode.bin
FLASH_9BC348251000_RETRYBIN=PS_SRTY\PS_SRTY_L06.bin

FLASH_9BC428492000_ISP=SM3281BB_ISP_TLC_YMTC.BIN
FLASH_9BC428492000_PTEST=PT.bin
FLASH_9BC428492000_BootCode=BootCode.bin
FLASH_9BC428492000_RETRYBIN=PS_SRTY\PS_SRTY_L06.bin
//---------------------------------------------------------------------//
